- Top
- Connecting to External Devices
- Connecting the remote operation panel (AK-HRP1000G/AK-HRP1005G)
- Serial connection with the <I/F> terminal

# Serial connection with the <I/F> terminal

AK-HRP1000G

AK-HRP1005G

<I/F> terminal

Connect the <I/F> terminal of this camera to the <CCU> terminal of the remote operation panel AK-HRP1000G/AK-HRP1005G.

Select [3] in [MAIN MENU] → [IN/OUT SELECT] → [PROTCOL] → [PROTCOL].

Set the [CONNECT SETTING] menu to [Serial(AW)] with the remote operation panel AK-HRP1000G/AK-HRP1005G.

For the functions that will operate, refer to the operating guide in following website.

http://pro-av.panasonic.net/

NOTE

- For the connection cable, refer to the “I/F cable specification” in “Details of the connector signals”. (I/F cable specification)

Top of the page