- Top
- Menu Operations
- Menu list
- [IN/OUT SELECT]

# [IN/OUT SELECT]

Item | Description of settings
--- | ---
[HD-SDI 3G SDI] | Sets the output format for HD SDI 3G output. [LEVEL-A], [LEVEL-B] Factory setting: [LEVEL-A]
[SDI1 OUT FMT] | Sets the output format of the <HD SDI OUT 1> terminal. When [FORMAT] is [2160/60p]: [1080/60p], [1080/60i], [720/60p] When [FORMAT] is [2160/59.94p]: [1080/59.94p], [1080/59.94i], [720/59.94p] When [FORMAT] is [2160/29.97p]: [1080/29.97PsF] When [FORMAT] is [2160/23.98p]: [1080/23.98p], [1080/23.98p over] When [FORMAT] is [2160/29.97PsF]: [1080/29.97PsF] When [FORMAT] is [2160/23.98PsF]: [1080/23.98PsF], [1080/23.98p over] When [FORMAT] is [2160/50p]: [1080/50p], [1080/50i], [720/50p] When [FORMAT] is [2160/25p]: [1080/25PsF] When [FORMAT] is [2160/25PsF]: [1080/25PsF] Factory setting: [1080/59.94p]
[HD-SDI1 CHAR] | Sets if the character is imposed to the output image of the <HD SDI OUT 1> terminal. [OFF], [ON] Factory setting: [OFF]
[HD-SDI OUT ITEM] | Sets the content of the character superimposed to the output image from the <HD SDI OUT 1>/<HD SDI OUT 2> terminal. [MENU ONLY]: Displays only on the menu. [STATUS]: Displays all characters that are the same as displayed in the monitor. Factory setting: [MENU ONLY]
[UHD-SDI S-LINK] | Switches the output signal when the 12G output board AK-UHD12G (optional) is installed. [ON]: Outputs the 12G SDI signal. [OFF]: Outputs the 3G SDI signal. Factory setting: [ON] Displayed only when the 12G output board AK-UHD12G (optional) is installed.
[UHD-SDI OUT TYPE] | Sets the output format of UHD. [SQUARE], [2 SAMPLE INT] Factory setting: [SQUARE]
[UHD-SDI 3G SDI] | Sets the output format for UHD SDI 3G output. [LEVEL-A], [LEVEL-B] Factory setting: [LEVEL-A]
[LAN CHAR] | Sets if the character is superimposed to the output signal from the <LAN> terminal. [OFF], [ON] Factory setting: [OFF]
[UHD CROP] | [HD-SDI2 OUT SEL] | Sets the output image of the <HD SDI OUT 2> terminal during cropping. [FULL], [CROP] Factory setting: [FULL]
| [LAN OUT SEL] | Sets the output image of the <LAN> terminal during cropping. [FULL], [CROP] Factory setting: [CROP]
| [CROP OUT SEL] | Sets the crop output image during cropping. [YL], [G], [MG] Factory setting: [YL]
| [CROP MARKER SEL] | Sets the crop frame to display during cropping. [YL], [G], [MG], [YL+G], [YL+MG], [G+MG], [YL+G+MG] Factory setting: [YL+G+MG]
| [CROP ADJ SEL] | Sets the crop frame to adjust the position during cropping. [YL], [G], [MG] Factory setting: [YL]
| [CROP H POSITION] | Sets the horizontal position of crop during cropping. [−50.00%] - [+50.00%] (0.25% steps) Factory setting: [0.00%]
| [CROP V POSITION] | Sets the vertical position of crop during cropping. [−50.00%] - [+50.00%] (0.25% steps) Factory setting: [0.00%]
[DISPLAY STATUS/BAR OSD] | [CAM ID SWITCH] | Sets the status display to superimpose in the main line signal. [OFF]: Camera ID is not displayed. [BAR]: Camera ID is displayed only when set to [BAR]. [ON]: Camera ID is constantly displayed. Factory setting: [OFF]
| [CAM ID CHARACTER] | Sets the camera name.
| [CAM ID POSI] | Sets the display position of the camera ID. [0]: Top left [1]: Top right [2]: Bottom left [3]: Bottom right Factory setting: [1]
[GEN-LOCK] | [GEN-LOCK INPUT] | Sets if the synchronization signal input is input from BNC or from D-SUB. [BNC], [DSUB] Factory setting: [BNC]
| [H PHASE-COARSE] | Roughly adjusts the phase of horizontal synchronization. [−5] - [+5] Factory setting: [0]
| [H PHASE-FINE] | Finely adjusts the phase of horizontal synchronization. [−100] - [+100] Factory setting: [0]
[PROTCOL] | [PROTCOL] | Sets the type of the protocol. [1]: Information camera communication protocol (EIA422) [2]: Information camera communication protocol (EIA232) [3]: Compatible personal computer control protocol (EIA422) [4]: Compatible personal computer control protocol (EIA232) Factory setting: [3]

Top of the page