- Top
- Description of Parts
- Rear side

# Rear side

1. Back tally lamp

   Lights up when the tally signal is supplied.

   Blinks in red while displaying warning, and blinks in green during the firmware update.

   NOTE

   - The brightness can be set with [MAIN MENU] → [SWITCH MODE] → [TALLY] → [BACK TALLY]. Blinks in green [LOW] regardless of setting during the firmware update.

2. <MENU> button

   Press this button to display the camera’s [MAIN MENU] screen.

   Press the button again to return to the original image.

3. Jog dial button

   This will perform the navigation of setting menu pages, and selection or setting of the item when the setting menu is displayed.

   The cursor will move down when the jog dial button is turned downward. The cursor will move up when turned upward.

   Press the jog dial button to fix the settings.

4. <I/F> terminal

   Connect the cable for the external synchronization signal and the control signal to the camera.

   For specification of the connection cable, refer to “Details of the connector signals”.

5. <LAN> terminal

   Used to connect the LAN cable.

   NOTE

   - Use a shielded cable when connecting a cable to the <LAN> terminal.

6. <WARNING> lamp

   This will illuminate in red when a problem occurs.

7. <IRIS> terminal

   Used to connect the lens iris control cable.

8. <TALLY OUT> terminal

   Outputs R tally and G tally.

9. <ZOOM/FOCUS> terminal

   Used to connect the lens zoom/focus control cable.

10. <HD SDI OUT 1> terminal

    This is the main line output terminal dedicated for HD SDI.

    NOTE

    - Use a cable that is 5C-FB or above.

11. <G/L IN> terminal

    This is the reference signal input terminal when applying external synchronization to the camera.

    NOTE

    - Supply a composite signal (black burst) or a tri-level SYNC as the input signal.

12. <HD SDI OUT 2> terminal

    This is the monitor output terminal dedicated for HD SDI.

    NOTE

    - Use a cable that is 5C-FB or above.

13. <DC IN> lamp

    This will illuminate in green when power is supplied to the camera.

14. <DC IN> terminal

    This is an input terminal for the external DC power supply. Connects to the external DC power supply. (DC 11 V to 17 V)

15. <UHD/HD SDI OUT 1>/<UHD/HD SDI OUT 2>/<UHD/HD SDI OUT 3>/<UHD/HD SDI OUT 4> terminal

    These are the UHD and HD SDI main line output terminals.

    NOTE

    - Use a cable that is 5C-FB or above.

Top of the page