- Top
- Web Screen
- [Setup] screen
- [Maintenance] screen

# [Maintenance] screen

Check system logs, confirm software versions, or initialize the camera.

The screen consists of three tabs, [Product info.], [Default reset], and [Back up].

## [Product info.] tab

Displays the software version of the camera.

Displays information of the camera such as [Model no.], [MAC address], [Serial no.], and [Firmware version].

Item | Description of settings
--- | ---
[Model no.] | Displays the model number of the camera.
[MAC address] | Displays the MAC address of the camera.
[Firmware version] | [VERSION]: Displays the system version of the camera. [CPU Software - CAM MAIN]: Displays the camera’s main software version. [CPU Software - NETWORK]: Displays the software version of the network component. [EEPROM - ROM TABLE]: Displays the version of the camera table. [FPGA - CAM FPGA]: Displays the camera’s FPGA version. [FPGA - AVIO FPGA]: Displays the FPGA version of the image processing component.
[Viewer software installation counter] | Displays the number of plugin software for display that has been installed automatically from the camera.
[Firmware file] | Updates the firmware.
[Status] | Displays the current status of the unit.

#### Update method of the firmware

Contact your dealer and download the latest software to the hard disc of the personal computer.

Click the [Browse...] button to specify the downloaded software.

Click the [Execute] button.

The confirmation screen of the update execution is displayed.

Always delete the Internet temporarily files after updating.

NOTE

- Space or double-byte character cannot be used as the save directory name.

- Make the total number of characters for the save directory name and the downloaded software name 250 characters or less.

- Always perform the update of the firmware from a personal computer within the same network (LAN) as the device to update.

- The time it takes for the progress bar to display the update processing after the [Execute] button is pressed is as follows.

  - CAM FPGA: Approx. one minute

  - NETWORK and AVIO FPGA: Approx. two minutes

  - Others: 30 seconds or less

- Use the following files specified by Panasonic as the software for update.

  - CPU Software - CAM MAIN

    RX_SOFT.srx

  - CPU Software – Network

    US2_SOFT.su2

  - EEPROM - ROM TABLE

    CAM_TABLE.eca

  - FPGA - CAM FPGA

    CAM_FPGA.fca

  - FPGA - AVIO FPGA

    AVIO_FPGA.fav

- Do not turn off the power of the unit during the update until the progress bar disappears.

- Do not perform any operation during the update until the update is completed.

## [Default reset] tab

Initialize the setting data of the camera and restart the camera.

Item | Description of settings
--- | ---
[Reset to the default (Except the network settings)] | By clicking the [Execute] button, resets the configuration of the camera to its default settings. The user name and password used for login are also reset to their default values (admin/12345). After executing the reset operation, the camera cannot be operated for approximately three minutes. The following setting items will not be reset. All items for [IPv4 network] [HTTP port] [Line speed] [Bandwidth control (bitrate)]
[Reboot] | Clicking the [Execute] button will restart the unit. Once the unit is restarted, it cannot be operated for approximately one minute as when the power of the unit is turned on.

## [Back up] tab

You can save network-related settings to a computer, or apply the settings saved in a computer to the camera.

Item | Description of settings
--- | ---
[Download] | Saves the network-related settings of the camera to a computer. (Saving the network-related settings of the camera to a computer ([Download]))
[Upload] | Uploads the setting file of the camera saved in a computer using the download function. (Applying the settings saved in a computer to the camera ([Upload]))

#### Saving the network-related settings of the camera to a computer ([Download])

Perform the following procedure to save the network-related settings of the camera to a computer.

Do not turn off the power of the camera while the download operation is in process.

Do not perform any operation from the start of the download operation until its end.

Click the [Execute] button for [Download].

A dialog box for saving destination appears.

Specify a saving destination folder, and then click the [OK] button.

The data will be saved.

#### Applying the settings saved in a computer to the camera ([Upload])

Perform the following procedure to upload the setting file of the camera saved in a computer using the download function [Download] to apply the settings to the camera.

Use the file downloaded with the camera when uploading data.

Do not change the extension (.ndt) of a downloaded file.

Do not turn off the power of the camera while the upload operation is in process.

Do not perform any operation from the start of the upload operation until its end.

Click the [Browse...] button on [Upload] to specify the downloaded setting file.

Click the [Execute] button.

A message dialog box appears.

Click the [OK] button.

Uploading will start.

When uploading has finished, a message dialog box appears.

Click the [OK] button.

The camera will be restarted automatically.

Top of the page