- Top
- UB300 Setting Tool
- Introduction
- Function of the UB300 Setting Tool

# Function of the UB300 Setting Tool

## Connection setting

It can connect to any AK-UB300G by setting the connection information.

The items that can be set are as follows.

#### Camera information

- IP address: Specify the IP address of AK-UB300G to connect.

- Port number: Specify the port number of AK-UB300G to connect. The default for camera side is 80.

#### Authentication information

- User name: Specify the account name with administrator privilege to be used at the time of connection.

- Password: Specify the password for the account with administrator privilege to be used at the time of connection.

#### Local host information

- Port number: Specify the port number that UB300 Setting Tool will use when it is to connect. It is not necessary to change if it is not required.

Once these items are set, click the [Connect] button to connect to the specified AK-UB300G.

## Firmware update function

Update can be performed on the connected AK-UB300G by specifying an arbitrary firmware.

The firmware that can be updated are as follows.

- CAM MAIN

- NETWORK

- ROM TABLE

- CAM FPGA

- AVIO FPGA

- Option (enabled only when an option board is added)

## Setting menu operation

Setting menu of the connected AK-UB300G can be operated.

The status of the displayed setting menu is synchronized with the connected AK-UB300G.

However, all setting menu items cannot be operated from this tool.

## OSD operation function

The buttons for OSD menu operation for AK-UB300G can be executed.

Use this when performing OSD operation while viewing the image output from AK-UB300G.

Top of the page