- Top
- Operation
- Convenient shooting functions
- UHD crop function

# UHD crop function

HD crop image from the UHD signal can be output to the <HD SDI OUT 1> terminal, <UHD/HD SDI OUT 1>/ <UHD/HD SDI OUT 2> terminal, and <LAN> terminal when [MAIN MENU] → [SYSTEM MODE] → [FORMAT] → [1080/59.94p CROP]/[1080/59.94i CROP]/[1080/50p CROP]/[1080/50i CROP] is selected (Fig. 2)

At this time, the HD signal with UHD aspect ratio is output to the image from the <HD SDI OUT 2> terminal, and crop frame is displayed. (Fig. 1)

To output the HD crop image to the image from the <HD SDI OUT 2> terminal, select [MAIN MENU] → [IN/OUT SELECT] → [UHD CROP] → [HD-SDI2 OUT SEL] → [CROP].

To display the crop frame of the UHD aspect ratio on the image from the <LAN> terminal, select [MAIN MENU] → [IN/OUT SELECT] → [UHD CROP] → [LAN OUT SEL] → [FULL].

Crop frame

Fig. 1

Fig. 2

- The cropped image to be output can be selected from three types in [MAIN MENU] → [IN/OUT SELECT] → [UHD CROP] → [CROP OUT SEL].

  The selected crop frame is displayed bright, and it is confirmed by pressing the jog dial.

  [YL]: Image of yellow crop frame is output.

  [G]: Image of green crop frame is output.

  [MG]: Image of magenta crop frame is output.

- Displaying of the crop frame can be selected in [MAIN MENU] → [IN/OUT SELECT] → [UHD CROP] → [CROP MARKER SEL].

  [YL]: Only the yellow crop frame is displayed.

  [G]: Only the green crop frame is displayed.

  [MG]: Only the magenta crop frame is displayed.

  [YL+G]: The yellow and green crop frames are displayed.

  [YL+MG]: The yellow and magenta crop frames are displayed.

  [G+MG]: The green and magenta crop frames are displayed.

  [YL+G+MG]: The yellow, green, and magenta crop frames are displayed.

  If the crop frame is overlapping in the same position, the crop frame selected in [CROP OUT SEL] will be prioritized, and then it is displayed in the order of [YL], [G], and [MG].

## To move the crop frame

- Selects the color of the crop frame in [MAIN MENU] → [IN/OUT SELECT] → [UHD CROP] → [CROP ADJ SEL].

  [YL]: Sets the position of yellow crop frame.

  [G]: Sets the position of green crop frame.

  [MG]: Sets the position of magenta crop frame.

- Sets the position of the crop frame in [MAIN MENU] → [IN/OUT SELECT] → [UHD CROP] → [CROP H POSITION]/[CROP V POSITION].

  [CROP H POSITION]: Moves horizontally.

  [CROP V POSITION]: Moves vertically.

NOTE

- The automatic functions such as the auto iris or the automatic white balance will operate in the UHD aspect ratio before cropping. The subject outside the crop frame may affect the cropped image when the auto function is operating.

- The setting of [MAIN MENU] → [PAINT] → [WHITE CLIP]/[DOWNCON DETAIL SETTING]/[SKIN TONE DETAIL SETTING] is not reflected to the image from the <HD SDI OUT 2> terminal or the <LAN> terminal when [FULL] is selected in [MAIN MENU] → [IN/OUT SELECT] → [UHD CROP] → [HD-SDI2 OUT SEL]/[LAN OUT SEL].

- When [MAIN MENU] → [PAINT] → [SKIN TONE DETAIL SETTING] → [SKIN GET] → [CURSOR] → [ON] is set in the UHD CROP mode, go through [MAIN MENU] → [IN/OUT SELECT] → [UHD CROP] → [HD-SDI2 OUT SEL]/[LAN OUT SEL], and select [CROP].

Top of the page