- Top
- Operation
- Adjustment for shooting
- Iris gain volume adjustment

# Iris gain volume adjustment

There is an iris gain adjustment hole (displayed as G or S) at the front of the lens housing. Adjust the iris gain volume inside the lens using a screwdriver.

#### Example for the iris automatic adjustment power zoom lens

1. Iris gain adjustment volume

Set the iris selection switch on the lens to A (AUTO) side.

Turn the iris gain adjustment volume so the gain will be at maximum in the range that will not cause hunting.

NOTE

- This can be adjusted with [MAIN MENU] → [SWITCH MODE] → [IRIS] → [IRIS SPEED] when set to [MAIN MENU] → [SWITCH MODE] → [IRIS] → [IRIS GAIN] → [CAM].

Top of the page