- Top
- Operation
- Adjustment for shooting
- Genlock adjustment

# Genlock adjustment

The video signal output from the camera can be locked to the reference signal supplied from an external source.

This camera can receive the external reference signal from the <G/L IN> terminal or the <I/F> terminal.

Select [MAIN MENU] → [IN/OUT SELECT] → [GEN-LOCK].

Select the input source of the synchronization signal in [GEN-LOCK INPUT].

Coarsely adjust the phase of the synchronization signal input and the video signal output in [H PHASE-COARSE].

Finely adjust the phase of the synchronization signal input and the video signal output in [H PHASE-FINE].

NOTE

- If the phase of the video output signal is adjusted using [H PHASE-COARSE] or [H PHASE-FINE] while the 12G output board AK-UHD12G is installed, the image output from the 12G output board AK-UHD12G may be interrupted for a moment. This is not a malfunction.

## External reference signal format

The external reference signal formats that each system format can apply genlock are as follows.

Genlock cannot be applied when there is no external reference signal input into the <G/L IN>terminal or the <I/F> terminal.

- ✓: Can lock.

- —: Cannot lock.

[MAIN MENU] | Input signal into the <G/L IN> terminal or the <I/F> terminal
--- | ---
[FORMAT] | 1080/60i | 1080/59.94i | 1080/50i | 1080/23PsF
[2160/60p] | ✓ | — | — | —
[2160/59.94p] | — | ✓ | — | —
[2160/50p] | — | — | ✓ | —
[2160/29.97p] | — | ✓ | — | —
[2160/29.97PsF] | — | ✓ | — | —
[2160/25p] | — | — | ✓ | —
[2160/25PsF] | — | — | ✓ | —
[2160/23.98p] | — | — | — | ✓
[2160/23.98PsF] | — | — | — | ✓
[1080/60p] | ✓ | — | — | —
[1080/59.94p] | — | ✓ | — | —
[1080/59.94p CROP] | — | ✓ | — | —
[1080/59.94i] | — | ✓ | — | —
[1080/59.94i CROP] | — | ✓ | — | —
[1080/50p] | — | — | ✓ | —
[1080/50p CROP] | — | — | ✓ | —
[1080/50i] | — | — | ✓ | —
[1080/50i CROP] | — | — | ✓ | —
[1080/29.97PsF] | — | ✓ | — | —
[1080/25PsF] | — | — | ✓ | —
[1080/23.98p] | — | ✓ | — | —
[1080/23.98PsF] | — | — | — | ✓
[720/60p] | — | — | — | —
[720/59.94p] | — | — | — | —
[720/50p] | — | — | — | —

[MAIN MENU] | Input signal into the <G/L IN> terminal or the <I/F> terminal
--- | ---
[FORMAT] | 720/60p | 720/59.94p | 720/50p | 525/59.94i | 625/50i
[2160/60p] | — | — | — | — | —
[2160/59.94p] | — | — | — | ✓ | —
[2160/50p] | — | — | — | — | ✓
[2160/29.97p] | — | — | — | ✓ | —
[2160/29.97PsF] | — | — | — | ✓ | —
[2160/25p] | — | — | — | — | ✓
[2160/25PsF] | — | — | — | — | ✓
[2160/23.98p] | — | — | — | — | —
[2160/23.98PsF] | — | — | — | — | —
[1080/60p] | — | — | — | — | —
[1080/59.94p] | — | — | — | ✓ | —
[1080/59.94p CROP] | — | — | — | ✓ | —
[1080/59.94i] | — | — | — | ✓ | —
[1080/59.94i CROP] | — | — | — | ✓ | —
[1080/50p] | — | — | — | — | ✓
[1080/50p CROP] | — | — | — | — | ✓
[1080/50i] | — | — | — | — | ✓
[1080/50i CROP] | — | — | — | — | ✓
[1080/29.97PsF] | — | — | — | ✓ | —
[1080/25PsF] | — | — | — | — | ✓
[1080/23.98p] | — | — | — | ✓ | —
[1080/23.98PsF] | — | — | — | — | —
[720/60p] | ✓ | — | — | — | —
[720/59.94p] | — | ✓ | — | ✓ | —
[720/50p] | — | — | ✓ | — | ✓

Top of the page