- Top
- Connecting to External Devices
- Connecting the remote camera controller (AW-RP50N/AW-RP50E/AW-RP120G)
- Serial connection with the <I/F> terminal

# Serial connection with the <I/F> terminal

AW-RP120G

AW-RP50N/AW-RP50E

<I/F> terminal

Connect the <I/F> terminal of this unit to the <TO PAN/TILT HEAD> terminal of the remote camera controller AW-RP50N/AW-RP50E/AW-RP120G.

Select [3] in [MAIN MENU] → [IN/OUT SELECT] → [PROTCOL] → [PROTCOL].

Set the remote camera controller to direct connection control (CAM_Direct).

NOTE

- For the connection cable, refer to the “I/F cable specification” in “Details of the connector signals”. (I/F cable specification)

#### Functions that can be controlled

Function | Description | Setting value
--- | --- | ---
GAIN | Switching the gain mode | [LOW], [MID], [HIGH], [S.GAIN1], [S.GAIN2], [S.GAIN3]
PED | Adjusting the master pedestal | [−99] - [+99]
R GAIN/B GAIN | Adjusting the Rch and Bch gains | [−1000] - [+1000]
R PED/B PED | Adjusting the Rch and Bch pedestals | [−800] - [+800]
AWB | Executing the automatic white balance | —
ABB | Executing the automatic black balance | —
SHUTTER | Switching the mode | [OFF], [STEP], [SYNCHRO]
Setting the step speed | For 59.94 Hz [1/100], [1/120], [1/125], [1/250], [1/500], [1/1000], [1/1500], [1/2000], [180.0deg], [172.8deg], [144.0deg], [120.0deg], [90.0deg], [45.0deg]
DETAIL | Switching enable/disable | —
MASTER DETAIL | Adjusting the master detail | [−31] - [+31]
SCENE | Loading the data | AW-RP50N/AW-RP50E: [CURRENT], [SCENE1] - [SCENE8] AW-RP120G: [CURRENT], [SCENE1] - [SCENE3] Corresponding buttons are as follows. <SCENE1> button: [CURRENT] <SCENE2> button: [SCENE1] <SCENE3> button: [SCENE2] <SCENE4> button: [SCENE3]
BARS | Switching the bar display | —
ND FILTER | Setting the ND filter | [CLEAR], [1/4], [1/16], [1/64]
AUTO | Enabling/disabling the auto iris | —
CAMERA OSD | Showing/hiding of the menu | —
EXIT (AW-RP50N/AW-RP50E only) | Going back 1 level of menu | —
IRIS | Adjusting the iris | —
ZOOM/FOCUS | Adjusting the zoom/focus | —
CROP OUT SEL | Setting the crop output image during cropping | [YL], [G], [MG]
CROP ADJ SEL | Setting the crop frame to adjust the position during cropping | [YL], [G], [MG]
CROP H/V POSITION | Adjusting the position of the crop frame during cropping | —

## Controlling the UHD cropping function

#### Controlling by AW-RP50N/AW-RP50E

Press the <MENU> button to illuminate the button.

Press the <9 SETUP> button in <PRESET MEMORY/MENU> to illuminate the button.

Turn the <F1> dial to display [[2] SW LINK] in the LCD panel, and press the <F1> dial.

Turn the <F1> dial to display [1.SWLINK], and select [Off] with the <F2> dial.

Press the <8 CAMERA> button in <PRESET MEMORY/MENU> to illuminate the button.

Turn the <F1> dial to display [[5] CROP] in the LCD panel, and press the <F1> dial.

Turn the <F1> dial to display [3.P/T LEVER], and select [CROP] with the <F2> dial.

Turn the <F1> dial to display [1.OUT SEL], and select the frame of the image to crop and output from [YL], [G], or [MG] with the <F2> dial.

Turn the <F1> dial to display [2.ADJ SEL], and select the frame of the image to adjust the crop position from [YL], [G], or [MG] with the <F2> dial.

Adjust the cropping position using the <PAN/TILT> lever and the <PTZ/FOCUS SPEED> dial.

#### Controlling by AW-RP120G

Press the <MENU> button to illuminate the button.

Press the <42 FUNCTION> button in <SWITCHER LINK> to illuminate the button.

Turn the <F1> dial to display [1.SWLINK] in the LCD panel, and select [Off] with the <F2> dial.

Press the <23 FUNCTION> button in <CAMERA OPERATION> to illuminate the button.

Turn the <F1> dial to display [12.CROP P/T LVR], and select [CROP] with the <F2> dial.

Turn the <F1> dial to display [10.CROP OUT SEL], and select the frame of the image to crop and output from [YL], [G], or [MG] with the <F2> dial.

Turn the <F1> dial to display [11.CROP ADJ SEL], and select the frame of the image to adjust the crop position from [YL], [G], or [MG] with the <F2> dial.

Adjust the position using the <PAN/TILT> lever and the <PAN/TILT SPEED> dial.

Top of the page