- Top
- Operation
- Multi-formats
- List of output formats (<UHD/HD SDI OUT 1> to <UHD/HD SDI OUT 4> terminals)

# List of output formats (<UHD/HD SDI OUT 1> to <UHD/HD SDI OUT 4> terminals)

Use following BNC cable in accordance to the signal to be output.

- 12G or 6G signal: 12G BNC cable

- Signal other than above: 5C-FB or higher BNC cable

## UHD

#### When the 12G output board AK-UHD12G is used, and [UHD-SDI S-LINK] is set to [ON]

- [UHD SDI OUT TYPE] and [HD-SDI 3G SDI] are displayed as [---], and cannot be selected.

[MAIN MENU] | <UHD/HD SDI OUT 1> to <UHD/HD SDI OUT 4> terminals
--- | ---
[FORMAT] | 1 | 2 | 3 | 4
[2160/60p] | 2160/60p (12GSL) | 2160/60p (12GSL) | No output
[2160/59.94p] | 2160/59.94p (12GSL) | 2160/59.94p (12GSL) | No output
[2160/29.97p] | 2160/29.97p (6GSL) | 2160/29.97p (6GSL) | No output
[2160/23.98p] | 2160/23.98p (6GSL) | 2160/23.98p (6GSL) | No output
[2160/50p] | 2160/50p (12GSL) | 2160/50p (12GSL) | No output
[2160/25p] | 2160/25p (6GSL) | 2160/25p (6GSL) | No output

#### When the 12G output board AK-UHD12G is used, and [UHD-SDI S-LINK] is set to [OFF], or when the standard equipment board is used

[MAIN MENU] | <UHD/HD SDI OUT 1> to <UHD/HD SDI OUT 4> terminals
--- | ---
[FORMAT] | [UHD SDI OUT TYPE] | 1, 2 | 3, 4
[2160/60p] | [SQARE] | 2160/60p (3GQL SQD)
| [2 SAMPLE INT] | 2160/60p (3GQL 2SI)
[2160/59.94p] | [SQARE] | 2160/59.94p (3GQL SQD)
| [2 SAMPLE INT] | 2160/59.94p (3GQL 2SI)
[2160/29.97p] | [SQARE] | 2160/29.97p (1.5GQL SQD)
| [2 SAMPLE INT] | 2160/29.97p (3GDL 2SI) | No output
[2160/23.98p] | [SQARE] | 2160/23.98p (1.5GQL SQD)
| [2 SAMPLE INT] | 2160/23.98p (3GDL 2SI) | No output
[2160/50p] | [SQARE] | 2160/50p (3GQL SQD)
| [2 SAMPLE INT] | 2160/50p (3GQL 2SI)
[2160/25p] | [SQARE] | 2160/25p (1.5GQL SQD)
| [2 SAMPLE INT] | 2160/25p (3GDL 2SI) | No output

#### When [FORMAT] is set to [2160/29.97PsF]/[2160/23.98PsF]/[2160/25PsF]

- [UHD-SDI S-LINK] and [UHD SDI OUT TYPE] are displayed as [---], and cannot be selected.

[MAIN MENU] | <UHD/HD SDI OUT 1> to <UHD/HD SDI OUT 4> terminals
--- | ---
[FORMAT] | 1 | 2 | 3 | 4
[2160/29.97PsF] | 2160/29.97PsF (1.5GQL SQD)
[2160/23.98PsF] | 2160/23.98PsF (1.5GQL SQD)
[2160/25PsF] | 2160/25PsF (1.5GQL SQD)

## UHD CROP

- [UHD-SDI S-LINK] will not display. Setting of [UHD SDI OUT TYPE] will be disabled.

[MAIN MENU] | <UHD/HD SDI OUT 1> to <UHD/HD SDI OUT 4> terminals
--- | ---
[FORMAT] | 1 | 2 | 3 | 4
[1080/59.94p CROP] | 1080/59.94p | 1080/59.94p | No output
[1080/59.94i CROP] | 1080/59.94i | 1080/59.94i | No output
[1080/50p CROP] | 1080/50p | 1080/50p | No output
[1080/50i CROP] | 1080/50i | 1080/50i | No output

## HD

- [UHD-SDI S-LINK] will not display. Setting of [UHD SDI OUT TYPE] will be disabled.

[MAIN MENU] | <UHD/HD SDI OUT 1> to <UHD/HD SDI OUT 4> terminals
--- | ---
[FORMAT] | 1 | 2 | 3 | 4
[1080/60p] | 1080/60p | 1080/60p | No output
[1080/59.94p] | 1080/59.94p | 1080/59.94p | No output
[1080/59.94i] | 1080/59.94i | 1080/59.94i | No output
[1080/29.97PsF] | 1080/29.97PsF | 1080/29.97PsF | No output
[1080/23.98PsF] | 1080/23.98PsF | 1080/23.98PsF | No output
[1080/23.98p] | 1080/23.98p over 59.94i | 1080/23.98p over 59.94i | No output
[1080/50p] | 1080/50p | 1080/50p | No output
[1080/50i] | 1080/50i | 1080/50i | No output
[1080/25PsF] | 1080/25PsF | 1080/25PsF | No output
[720/60p] | 720/60p | 720/60p | No output
[720/59.94p] | 720/59.94p | 720/59.94p | No output
[720/50p] | 720/50p | 720/50p | No output

Top of the page