- Top
- Picture monitor (PM)
- Information display
- IRIS display

# IRIS display

When the information is not displayed on the picture monitor, display it by pressing the [CHARA] button of the ROP.

A.Camera number

B.IRIS F value

C.IRIS level

D.IRIS memory

E.TALLY INFO

- Set each item to be displayed on the [PM VIEW SETTING] screen that can be accessed by selecting [MAINTENANCE] on the CCU menu. However, this screen will not appear if the menu's [IRIS LEVEL] setting is [OFF].

- The IRIS schedule is displayed as follows depending on the setting of [IRIS SCALE] that can be accessed by selecting [MAINTENANCE] > [SETUP].

IRIS SCALE: FULL

IRIS SCALE: 2STOP

In the IRIS level display, the IRIS F value stored in IRIS memory is indicated at the center (+), and the current IRIS F value is displayed relative to the center as "".

When the center value (+) and the current IRIS value () overlap, the display shows " ".

When the IRIS level falls outside either end of the display range, the status is displayed as a flashing "" or "".

- TALLY INFO (E)

Display the R tally in two segments of the upper row and the R, G, or YL tally in two segments of the lower row.

When all R, G, and YL tally signals are ON, the upper row is red, and the left and right segments of the lower row are green and yellow, respectively.

When the R and G tally signals are ON, the upper row is red and the lower row is green.

Top of the page