- Top
- CCU menu
- OPERATION
- SETTING(MOIP)

# SETTING(MOIP)

This is the selection screen for the SETTING(MOIP).

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
SELECT HD PROMPT | SDI SFP+ | Selects the input connector for HD prompter signals.
SELECT REF SIGNAL | SDI PTP | Selects the input connector for reference signals.
SELECT AUDIO SIGNAL | NORMAL SFP+ | Selects the input/output connector for audio signals.
SELECT RETURN SIGNAL | SDI SFP+ | Selects the input connector for the return signals.

Top of the page