- Top
- CCU menu
- OPERATION
- OUT FORMAT(HS_HDR)

# OUT FORMAT(HS_HDR)

This is the selection screen for the OUT FORMAT(HS_HDR) menu.

- This is not displayed when AK-PLV100 is connected.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
SDI OUT1-4 | HS_3G_HDR HS_HD_HDR | Displays the format of the signals to be output from [1] to [4] of the [UHD/HS/HD SDI OUT] connectors.
SDI OUT5&6 | 3G_HDR HD_HDR 3G_SDR HD_SDR | Set the format of the signals to be output from [5] to [6] of the [HD SDI OUT] connectors.
SDI OUT7 | 3G_HDR HD_HDR 3G_SDR HD_SDR | Set the format of the signals to be output from [7] of the [HD SDI OUT] connector.
SDI OUT8 | HD_HDR HD_SDR | Displays the format of the signals to be output from [8/PM] of the [HD SDI OUT] connectors.
SDI OUT8 NORMAL/PM | PM NORMAL | Set the signal to be output from [8/PM] of the [HD SDI OUT] connector. Can only be set to PM when using a MoIP board (AK-NP600). PM : Output the picture monitor images. NORMAL : Output the main line images.
3G SDI | LEVEL-A LEVEL-B | Set the output format for 3G output.
HD SDI FORMAT | 1080i 720P | Set the format for HD output.
HDR COLORIMETRY | BT.709 BT.2020 | Switches the Y/C conversion coefficient.
HDR GAMUT | NORMAL WIDE_G WIDE_G2 | Switches the color gamut. Only signals output from the [SDI OUT 1] to [SDI OUT 4] connectors are switched. This will be NORMAL/WIDE_G when AK-UC3000 is connected.

#### Output selection conditions

FORMAT/ CCU MODE | SDI | ANALOG
--- | --- | ---
OUT1 | OUT2 | OUT3 | OUT4 | OUT5 | OUT6 | OUT7 | OUT8 | COMPOSITE /PM
HS_HDR(59.94)
| 1080/59.94p-240fps | HS_3G_HDR,HS_HD_HDR | 3G_HDR,3G_SDR,HD_HDR,HD_SDR | HD_HDR,HD_SDR | NORMAL /PM
1080/59.94p-180fps | HS_3G_HDR,HS_HD_HDR | no signal | 3G_HDR,3G_SDR,HD_HDR,HD_SDR | HD_HDR,HD_SDR | NORMAL /PM
1080/59.94p-120fps | HS_3G_HDR,HS_HD_HDR | no signal | 3G_HDR,3G_SDR,HD_HDR,HD_SDR | HD_HDR,HD_SDR | NORMAL /PM
720/59.94p-240fps | HD_HDR | HD_HDR,HD_SDR | NORMAL /PM
720/59.94p-180fps | HD_HDR | no signal | HD_HDR,HD_SDR | NORMAL /PM
720/59.94p-120fps | HD_HDR | no signal | HD_HDR,HD_SDR | NORMAL /PM
HS_HDR(50)
| 1080/50p-200fps | HS_3G_HDR,HS_HD_HDR | 3G_HDR,3G_SDR,HD_HDR,HD_SDR | HD_HDR,HD_SDR | NORMAL /PM
1080/50p-150fps | HS_3G_HDR,HS_HD_HDR | no signal | 3G_HDR,3G_SDR,HD_HDR,HD_SDR | HD_HDR,HD_SDR | NORMAL /PM
1080/50p-100fps | HS_3G_HDR,HS_HD_HDR | no signal | 3G_HDR,3G_SDR,HD_HDR,HD_SDR | HD_HDR,HD_SDR | NORMAL /PM
720/50p-200fps | HD_HDR | HD_HDR,HD_SDR | NORMAL /PM
720/50p-150fps | HD_HDR | no signal | HD_HDR,HD_SDR | NORMAL /PM
720/50p-100fps | HD_HDR | no signal | HD_HDR,HD_SDR | NORMAL /PM

Top of the page