- Top
- CCU menu
- OPERATION
- BAR ID

# BAR ID

This is the selection screen for the BAR ID menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
BAR ID SWITCH | ON OFF | Set display of the camera ID in the color bar ON or OFF.
BRIGHTNESS | 0 to 100% | Set the text color for the camera ID in the color bar. The setting can be made in 10% steps. 0 : Black 100%: White
ID1 POSITION V | 00 to 05 | Set the starting position (vertical) for display of camera ID1 in the color bar. Set from which character in the vertical direction, starting from the top left of the color bar, to start displaying the BAR ID using the font size as the reference.
ID1 POSITION H | 00 to 15 | Set the starting position (horizontal) for display of camera ID1 in the color bar. Set from which character in the horizontal direction in the color bar to start displaying the BAR ID using the font size as the reference.
ID1 | ## (Max. 16 characters) | Set camera ID1. This ID is displayed in the color bar. Characters which can be used: Alphanumeric characters, spaces, ! # % & ' ( ) * + , - . / : ; < = > ? [ ] _ ~ If "##" is input, that portion is replaced with the camera number (1 to 15) being managed by the CCU.
ID2 POSITION V | 00, 01 to 05 | Set the starting position (vertical) for display of camera ID2 in the color bar. Set from which character in the vertical direction, starting from the top left of the color bar, to start displaying the BAR ID using the font size as the reference.
ID2 POSITION H | 00 to 15 | Set the starting position (horizontal) for display of camera ID2 in the color bar. Set from which character in the horizontal direction in the color bar to start displaying the BAR ID using the font size as the reference.
ID2 | Spaces (Max. 16 characters) | Set camera ID2. This ID is displayed in the color bar. Characters which can be used: Alphanumeric characters, spaces, ! # % & ' ( ) * + , - . / : ; < = > ? [ ] _ ~ If "##" is input, that portion is replaced with the camera number (1 to 99) being managed by the CCU.
OFFSET V | 00 to 89 | Specify the origin (upper left) in the vertical direction of the character drawing area in pixels.
OFFSET H | 00 to 79 | Specify the origin (upper left) in the horizontal direction of the character drawing area in pixels.
HS PHASE MARKER SW | ON OFF | Set whether PHASE MARKER is multiplexed in the color bar when HS is set.

NOTE

- When the coordinates of ID1 and ID2 are the same, BAR ID1’s character string will be placed on top of BAR ID2 (BAR ID2 will be on the bottom). When the vertical coordinates are the same and the horizontal coordinates differ, the BAR ID with the horizontal coordinates set later will be placed on top.

Top of the page