- Top
- CCU menu
- UHD SETTING
- UHD SKIN TONE DETAIL(2/2)

# UHD SKIN TONE DETAIL(2/2)

This is the selection screen for the UHD SKIN TONE DETAIL(2/2) menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
I CENTER | 000 to 87 to 255 | Set the center position (area to which skin tone is applied) on the I axis.
I WIDTH | 000 to 20 to 255 | Set the width of the area to which skin tone is applied on the I axis using the [I CENTER] setting as the center.
Q WIDTH | 000 to 43 to 255 | Set the width of the area to which skin tone is applied on the Q axis using the [I CENTER] setting as the center.
Q PHASE | 0 to 90 to 359 | Set the phase of the area to which the skin tone effect is applied, with the Q axis being the reference.

Top of the page