- Top
- Introduction
- Precautions for Installation
- Mounting the unit in a rack

# Mounting the unit in a rack

#### Mounting the rack mount adapters

1.Remove the setting legs (A) secured to the unit.

Remove them using a Phillips screwdriver.

2.Mount the supplied rack mount adapters (B).

- Mounting screws are not supplied. Use mounting screws removed from the unit using a Phillips screwdriver.

Tighten the mounting screws for rack mount adapters using a torque of 110 N·m or more.

A.Setting legs

B.Rack mount adapters

#### Mounting the unit in a rack

- Use the unit securely mounted in a standard 19-type rack (depth: 600 mm [23-5/8 inches] or more) compliant with EIA or JIS standards or equivalent.

- Securely fix the unit in place using screws that are appropriate for the rack.

- Be sure to attach a support guide for supporting (A) the rear of the unit.

(Provide a support guide that is appropriate for the rack.)

A.Support guide

#### Mounting positions

In the case of the EIA standard rack | In the case of the JIS standard rack

NOTE

- Do not block the ventilation holes when installing the unit.

Top of the page