- Top
- CCU menu
- MAINTENANCE
- SYSTEM

# SYSTEM

This is the selection screen for the SYSTEM menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
INITIALIZE | - | Return the menu items to the factory default values. “Initialize the Unit Settings (INITIALIZE)”
FACTORY INITIALIZE | - | Return the unit's settings to the factory default values. When you place the cursor on [FACTORY INITIALIZE] and press the [SELECT] dial, [FACTORY INITIALIZE? NO/YES] appears. Select [YES] to start initialization. Controls from the camera, ROP, or MSU cannot be performed during initialization.
CCU CUSTOM DATA LOAD | ------- | Call the CCU management data stored in the CCU.
CCU CUSTOM DATA SAVE | CURRENT FACTORY CANCEL | Store the setting data managed by the CCU inside the CCU. The items that are stored are the same as the items set with [FACTORY INITIALIZE]. CURRENT Saves the values currently set for the CCU. FACTORY Saves the values set with [FACTORY INITIALIZE].
ROP CONNECT SERIAL | FRONT REAR ------- | Displays the status of ROP connection (serial connection) to the unit. FRONT Connection is to the front panel [ROP] connector. REAR Connection is to the rear panel [ROP] connector. ------- No serial connection.
ROP CONNECT NETWORK | CONNECT ------- | Displays the status of ROP connection (IP connection) to the unit. CONNECT Connection is by IP connection. ------- No IP connection.

#### Initialize the Unit Settings (INITIALIZE)

#### Initialization Procedure

1.Turn the [SELECT] dial to move the cursor to [INITIALIZE], and then press the [SELECT] dial.

2.Turn the [SELECT] dial to select [YES?], and then press the [SELECT] dial.

Initialization begins.

#### Data Initialized

: Initialized ×: Not initialized

CCU menu | INITIALIZE | FACTORY INITIALIZE
--- | --- | ---
OPERATION |  |
UHD SETTING |  |
AUDIO |  |
MAINTENANCE
START UP | (excluding [CONNECT MODE]) |
SETUP | (excluding [ROP SW]) |
AUX |  |
ANALOG GAIN |  |
ND/CC NAME |  |
NETWORK | × |
VERSION | × | ×
PM VIEW SETTING |  |
PM OPERATION STATUS |  |
SYSTEM | × | ×
SD CARD | × | ×

Top of the page