- Top
- CCU menu
- MAINTENANCE
- START UP

# START UP

This is the selection screen for the START UP menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
CAM POWER | OFF ON REMOTE | Set the control of the camera's power that is to be performed when the unit's power is turned on. OFF The camera's power will not come on even when the unit's power is turned on. In this case, "HEAD POWER" on the operation panel of the ROP or [CAMERA POWER] on the unit must be set to ON. ON The camera's power will come on when the unit's power is turned on. REMOTE Turns on in the same state as when the CCU power was turned OFF.
VF POWER | OFF ON REMOTE | Set the control of the viewfinder's power that is performed when the unit's power is turned on. OFF The viewfinder's power will not come on even when the unit's power is turned on. In this case, "VF POWER" must be set to ON on the operation panel of the ROP. ON Turning on the power of this unit also turns on the power of the viewfinder. REMOTE Turns on in the same state as when the CCU power was turned OFF.
CONNECT MODE | UC4000 UC3000 UC3300 | Set the unit to connect to AK-UC4000, AK-UC3000, or AK-UC3300 when turning on the power of this unit. UC4000 Connect to the AK-UC4000. UC3000 Connect to the AK-UC3000. UC3300 Connect to the AK-UC3300.

Top of the page