- Top
- CCU menu
- UHD SETTING
- UHD DETAIL

# UHD DETAIL

This is the selection screen for the UHD DETAIL menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
UHD DTL SW | OFF ON | Enable/disable the detail function.
MASTER DTL | -31 to 0 to +31 | Set the master detail.
H-DETAIL | 0 to 20 to 63 | Set the horizontal detail correction level.
V-DETAIL | 0 to 32 to 63 | Set the vertical detail correction level.
CRISP | 0 to 5 to 63 | Set the noise elimination level for the detail signals.
PEAK | 1 to 4 to 5 | Set the peak frequency of the horizontal detail.
DETAIL CLIP+ | 00 to +63 | Adjust detail clipping to minimize any roughness that results from excessive detail application.
DETAIL CLIP- | 00 to +63 | This limits the length of the undershoot portion of the detail edge component.
KNEE APERTURE LEVEL | 00 to 39 | Adjust the knee aperture level. For HDR format, this is fixed at [5].
DETAIL KNEE | 00 to 15 | Adjust the knee detail component.
LEVEL DEPENDENT SWITCH | OFF ON | Enable/disable the function for removing details in dark areas. For HDR format, this is fixed at [OFF].
LEVEL DEPENDENT | 00 to 8 to 15 | Set the level of dark detail removal.
DARK DETAIL SWITCH | OFF ON | Enable/disable the function for enhancing details in dark areas. For HDR format, this is fixed at [OFF].
DARK DETAIL | 0 to 7 | Set the level of dark detail enhancement.

Top of the page