- Top
- Picture monitor (PM)
- Information display
- Auto displays

# Auto displays

When the following operation is performed while no menu is displayed on the picture monitor, information on the operation performed appears at the bottom of the screen.

- AWB (Auto White Balance) function

- ABB (Auto Black Balance) function

- AUTO SETUP (Auto Setup) function

- The AUTO SETUP function does not work when AK-PLV100 is connected.

When the AUTO SETUP operations are displayed, they will remain displayed until the operations are completed.

The display is cleared 4 seconds after the operations are completed.

If the operations cannot be completed, they will remain displayed until the NG (error) items of the AUTO function are released.

The display time can be changed from [MAINTENANCE] menu > [PM OPERATION STATUS] > [STATUS DISP TIME].

Item | Display description
--- | ---
AWB | AWB : OK
AWB : ACTIVE
AWB : G/B/R NG
AWB : BREAK
ABB | ABB : OK
ABB : ACTIVE
ABB : G/B/R NG
ABB : LENS OPEN
ABB : BREAK
AUTO SETUP | AUTO SETUP : OK (Details on the operation are displayed at the bottom.)
AUTO SETUP : NG (Details on the NG information are displayed at the bottom.)
AUTO SETUP : BREAK

- AUTO SETUP operation details

Display description
B.SHD OPERATION
W.SHD OPERATION
GAMMA OPERATION
FLARE OPERATION
AWB OPERATION
ABB OPERATION
NOT RUNNING ILLEGAL MODE

Top of the page