- Top
- CCU menu
- MAINTENANCE
- NETWORK(MOIP)

# NETWORK(MOIP)

This is the selection screen for the NETWORK(MOIP) menu.

Item | Content
--- | ---
SFP+ PRIMARY | Displays the SFP+ PRIMARY setting menu.
SFP+ PRIMARY TX | Displays the SFP+ PRIMARY TX signal setting menu.
SFP+ PRIMARY RX | Displays the SFP+ PRIMARY RX signal setting menu.
SFP+ SECONDARY | Displays the SFP+ SECONDARY setting menu.
SFP+ SECONDARY TX | Displays the SFP+ SECONDARY TX signal setting menu.
SFP+ SECONDARY RX | Displays the SFP+ SECONDARY RX signal setting menu.
1GbE | Displays the 1GbE (LAN2) setting menu.
TALLY IN SETTING | Displays the TALLY IN setting menu.
PTP SETTING | Displays the PTP setting menu.
NMOS SETTING | Displays the NMOS setting menu.

#### NETWORK(SFP+ PRM)

This is the selection screen for the NETWORK(SFP+ PRM) menu.

Item | Setting value | Setting details
--- | --- | ---
main
DHCP | OFF, ON (Factory setting: OFF) | Enables/disables DHCP.
IP ADDR | (Factory setting: 192.168.0.50) | Sets the PORT for SFP+ primary.
PORT | (Factory setting: 49300) | Sets the PORT for SFP+ primary.
SUBNETMASK | (Factory setting: 255.255.255.0) | Sets the subnet mask.
DEFAULT GATEWAY | (Factory setting: 192.168.0.1) | Sets the default gateway.
SET EXECUTE | - | When you press the [SELECT] button, [NETWORK(PRM) SET EXECUTE NO/YES] appears. Select [YES] to apply the configured [NETWORK(SFP+ PRM)] information to the unit. If this operation is not performed, the changed [NETWORK(SFP+ PRM)] settings will not be applied. In addition, if you exit the menu without performing this operation, the settings will return to their original values.
MAC ADDR | Display only | Displays the MAC address.

#### NETWORK(SFP+ PRM TX)

This is the selection screen for the NETWORK(SFP+ PRM TX)) menu.

Item | Setting value | Setting details
--- | --- | ---
MAIN VIDEO TX | This is the setting for the main line output video.
IP ADDR | (Factory setting: 224.1.0.1) | Sets the IP address for MAIN VIDEO TX.
PORT | 01024 to 65535 (Factory setting: 49301) (Setting 10670 is prohibited.) | Sets the PORT for MAIN VIDEO TX.
MONITOR VIDEO TX | This is the setting for the monitor output video.
IP ADDR | (Factory setting: 224.1.0.2) | Sets the IP address for MONITOR VIDEO TX.
PORT | 01024 to 65535 (Factory setting: 49302) (Setting 10670 is prohibited.) | Sets the PORT for MONITOR VIDEO TX.
HD TRUNK TX | This is the setting for the HD TRUNK TX.
IP ADDR | (Factory setting: 224.1.0.10) | Sets the IP address for HD TRUNK TX.
PORT | 01024 to 65535 (Factory setting: 49310) (Setting 10670 is prohibited.) | Sets the PORT for HD TRUNK TX.
MIC1 AUDIO TX | This is the setting for the MIC1 output.
IP ADDR | (Factory setting: 224.1.0.3) | Sets the IP address for MIC1 AUDIO TX.
PORT | 01024 to 65535 (Factory setting: 49303) (Setting 10670 is prohibited.) | Sets the PORT for MIC1 AUDIO TX.
MIC2 AUDIO TX | This is the setting for the MIC2 output.
IP ADDR | (Factory setting: 224.1.0.11) | Sets the IP address for MIC2 AUDIO TX.
PORT | 01024 to 65535 (Factory setting: 49311) (Setting 10670 is prohibited.) | Sets the PORT for MIC2 AUDIO TX.
INCOM1 AUDIO TX | This is the setting for the INCOM1 output.
IP ADDR | (Factory setting: 224.1.0.12) | Sets the IP address for INCOM1 AUDIO TX.
PORT | 01024 to 65535 (Factory setting: 49312) (Setting 10670 is prohibited.) | Sets the PORT for INCOM1 AUDIO TX.
INCOM2 AUDIO TX | This is the setting for the INCOM2 output.
IP ADDR | (Factory setting: 224.1.0.13) | Sets the IP address for INCOM2 AUDIO TX.
PORT | 01024 to 65535 (Factory setting: 49313) (Setting 10670 is prohibited.) | Sets the PORT for INCOM2 AUDIO TX.
SET EXECUTE | - | When you press the [SELECT] button, [NETWORK(PRM TX) SET EXECUTE NO/YES] appears. Select [YES] to apply the configured [NETWORK(SFP+ PRM TX)] information to the unit. If this operation is not performed, the changed [NETWORK(SFP+ PRM TX)] settings will not be applied. In addition, if you exit the menu without performing this operation, the settings will return to their original values.

#### NETWORK(SFP+ PRM RX)

This is the selection screen for the NETWORK(SFP+ PRM RX) menu.

Item | Setting value | Setting details
--- | --- | ---
RET VIDEO RX | This is the setting for the return video input.
MCAST ADDR | (Factory setting: 224.1.0.4) | Set to 0.0.0.0 if no limitations on multicast source are to be implemented. If you want to establish a source address, set the relevant address.
SOURCE ADDR | (Factory setting: 0.0.0.0) | Sets the PORT for RET VIDEO RX.
PORT | 01024 to 65535 (Factory setting: 49304) (Setting 10670 is prohibited.) | Sets the PORT for RET VIDEO RX.
HD PROMPTER RX | This is the setting for the HD PROMPTER input.
MCAST ADDR | (Factory setting: 224.1.0.14) | Sets the IP address for HD PROMPTER RX.
SOURCE ADDR | (Factory setting: 0.0.0.0) | Set to 0.0.0.0 if no limitations on multicast source are to be implemented. If you want to establish a source address, set the relevant address.
PORT | 01024 to 65535 (Factory setting: 49314) (Setting 10670 is prohibited.) | Sets the PORT for HD PROMPTER RX.
SET EXECUTE | - | When you press the [SELECT] button, [NETWORK(PRM RX) SET EXECUTE NO/YES] appears. Select [YES] to apply the configured [NETWORK(SFP+ PRM RX)] information to the unit. If this operation is not performed, the changed [NETWORK(SFP+ PRM RX)] settings will not be applied. In addition, if you exit the menu without performing this operation, the settings will return to their original values.
PGM1 AUDIO RX | This is the setting for the PGM1 input.
MCAST ADDR | (Factory setting: 224.1.0.16) | Sets the IP address for PGM1 AUDIO RX.
SOURCE ADDR | (Factory setting: 0.0.0.0) | Set to 0.0.0.0 if no limitations on multicast source are to be implemented. If you want to establish a source address, set the relevant address.
PORT | 01024 to 65535 (Factory setting: 49316) (Setting 10670 is prohibited.) | Sets the PORT for PGM1 AUDIO RX.
PGM2 AUDIO RX | This is the setting for the PGM2 input.
MCAST ADDR | (Factory setting: 224.1.0.17) | Sets the IP address for PGM2 AUDIO RX.
SOURCE ADDR | (Factory setting: 0.0.0.0) | Set to 0.0.0.0 if no limitations on multicast source are to be implemented. If you want to establish a source address, set the relevant address.
PORT | 01024 to 65535 (Factory setting: 49317) (Setting 10670 is prohibited.) | Sets the PORT for PGM2 AUDIO RX.
SET EXECUTE | - | When you press the [SELECT] button, [NETWORK(PRM RX) SET EXECUTE NO/YES] appears. Select [YES] to apply the configured [NETWORK(SFP+ PRM RX)] information to the unit. If this operation is not performed, the changed [NETWORK(SFP+ PRM RX)] settings will not be applied. In addition, if you exit the menu without performing this operation, the settings will return to their original values.
INCOM1 AUDIO RX | This is the setting for the INCOM1 input.
MCAST ADDR | (Factory setting: 224.1.0.18) | Sets the IP address for INCOM1 AUDIO RX.
SOURCE ADDR | (Factory setting: 0.0.0.0) | Set to 0.0.0.0 if no limitations on multicast source are to be implemented. If you want to establish a source address, set the relevant address.
PORT | 01024 to 65535 (Factory setting: 49318) (Setting 10670 is prohibited.) | Sets the PORT for INCOM1 AUDIO RX.
INCOM2 AUDIO RX | This is the setting for the INCOM2 input.
MCAST ADDR | (Factory setting: 224.1.0.19) | Sets the IP address for INCOM2 AUDIO RX.
SOURCE ADDR | (Factory setting: 0.0.0.0) | Set to 0.0.0.0 if no limitations on multicast source are to be implemented. If you want to establish a source address, set the relevant address.
PORT | 01024 to 65535 (Factory setting: 49319) (Setting 10670 is prohibited.) | Sets the PORT for INCOM2 AUDIO RX.
SET EXECUTE | - | When you press the [SELECT] button, [NETWORK(PRM RX) SET EXECUTE NO/YES] appears. Select [YES] to apply the configured [NETWORK(SFP+ PRM RX)] information to the unit. If this operation is not performed, the changed [NETWORK(SFP+ PRM RX)] settings will not be applied. In addition, if you exit the menu without performing this operation, the settings will return to their original values.

#### NETWORK(SFP+ SCD)

This is the selection screen for the NETWORK(SFP+ SCD) menu.

Item | Setting value | Setting details
--- | --- | ---
main
DHCP | OFF, ON (Factory setting: OFF) | Enables/disables DHCP.
IP ADDR | (Factory setting: 192.168.0.51) | Sets the IP address for SFP+ SECONDARY.
PORT | (Factory setting: 49309) | Sets the PORT for SFP+ SECONDARY.
SUBNETMASK | (Factory setting: 255.255.255.0) | Sets the subnet mask.
DEFAULT GATEWAY | (Factory setting: 192.168.0.1) | Sets the default gateway.
SET EXECUTE | - | When you press the [SELECT] button, [NETWORK(SCD) SET EXECUTE NO/YES] appears. Select [YES] to apply the configured [NETWORK(SFP+ SCD)] information to the unit. If this operation is not performed, the changed [NETWORK(SFP+ SCD)] settings will not be applied. In addition, if you exit the menu without performing this operation, the settings will return to their original values.
MAC ADDR | Display only | Displays the MAC address.

#### NETWORK(SFP+ SCD TX)

This is the selection screen for the NETWORK(SFP+ SCD TX) menu.

Item | Setting value | Setting details
--- | --- | ---
MAIN VIDEO TX | This is the setting for the main line output video.
IP ADDR | (Factory setting: 224.1.0.5) | Sets the IP address for MAIN VIDEO TX.
PORT | 01024 to 65535 (Factory setting: 49305) (Setting 10670 is prohibited.) | Sets the PORT for MAIN VIDEO TX.
MONITOR VIDEO TX | This is the setting for the monitor output video.
IP ADDR | (Factory setting: 224.1.0.6) | Sets the IP address for MONITOR VIDEO TX.
PORT | 01024 to 65535 (Factory setting: 49306) (Setting 10670 is prohibited.) | Sets the PORT for MONITOR VIDEO TX.
HD TRUNK TX | This is the setting for the HD TRUNK TX.
IP ADDR | (Factory setting: 224.1.0.20) | Sets the IP address for HD TRUNK TX.
PORT | 01024 to 65535 (Factory setting: 49320) (Setting 10670 is prohibited.) | Sets the PORT for HD TRUNK TX.
MIC1 AUDIO TX | This is the setting for the MIC1 output.
IP ADDR | (Factory setting: 224.1.0.7) | Sets the IP address for MIC1 AUDIO TX.
PORT | 01024 to 65535 (Factory setting: 49307) (Setting 10670 is prohibited.) | Sets the PORT for MIC1 AUDIO TX.
MIC2 AUDIO TX | This is the setting for the MIC2 output.
IP ADDR | (Factory setting: 224.1.0.21) | Sets the IP address for MIC2 AUDIO TX.
PORT | 01024 to 65535 (Factory setting: 49321) (Setting 10670 is prohibited.) | Sets the PORT for MIC2 AUDIO TX.
INCOM1 AUDIO TX | This is the setting for the INCOM1 output.
IP ADDR | (Factory setting: 224.1.0.22) | Sets the IP address for INCOM1 AUDIO TX.
PORT | 01024 to 65535 (Factory setting: 49322) (Setting 10670 is prohibited.) | Sets the PORT for INCOM1 AUDIO TX.
INCOM2 AUDIO TX | This is the setting for the INCOM2 output.
IP ADDR | (Factory setting: 224.1.0.23) | Sets the IP address for INCOM2 AUDIO TX.
PORT | 01024 to 65535 (Factory setting: 49323) (Setting 10670 is prohibited.) | Sets the PORT for INCOM2 AUDIO TX.
SET EXECUTE | - | When you press the [SELECT] button, [NETWORK(SCD TX) SET EXECUTE NO/YES] appears. Select [YES] to apply the configured [NETWORK(SFP+ SCD TX)] information to the unit. If this operation is not performed, the changed [NETWORK(SFP+ SCD TX)] settings will not be applied. In addition, if you exit the menu without performing this operation, the settings will return to their original values.

#### NETWORK(SFP+ SCD RX)

This is the selection screen for the NETWORK(SFP+ SCD RX) menu.

Item | Setting value | Setting details
--- | --- | ---
RET VIDEO RX | This is the setting for the return video input.
MCAST ADDR | (Factory setting: 224.1.0.8) | Sets the IP address for RET VIDEO RX.
SOURCE ADDR | (Factory setting: 0.0.0.0) | Set to 0.0.0.0 if no limitations on multicast source are to be implemented. If you want to establish a source address, set the relevant address.
PORT | 01024 to 65535 (Factory setting: 49308) (Setting 10670 is prohibited.) | Sets the PORT for RET VIDEO RX.
HD PROMPTER RX | This is the setting for the HD PROMPTER input.
MCAST ADDR | (Factory setting: 224.1.0.24) | Sets the IP address for HD PROMPTER RX.
SOURCE ADDR | (Factory setting: 0.0.0.0) | Set to 0.0.0.0 if no limitations on multicast source are to be implemented. If you want to establish a source address, set the relevant address.
PORT | 01024 to 65535 (Factory setting: 49324) (Setting 10670 is prohibited.) | Sets the PORT for HD PROMPTER RX.
SET EXECUTE | - | When you press the [SELECT] button, [NETWORK(SCD RX) SET EXECUTE NO/YES] appears. Select [YES] to apply the configured [NETWORK(SFP+ SCD RX)] information to the unit. If this operation is not performed, the changed [NETWORK(SFP+ SCD RX)] settings will not be applied. In addition, if you exit the menu without performing this operation, the settings will return to their original values.
PGM1 AUDIO RX | This is the setting for the PGM1 input.
MCAST ADDR | (Factory setting: 224.1.0.26) | Sets the IP address for PGM1 AUDIO RX.
SOURCE ADDR | (Factory setting: 0.0.0.0) | Set to 0.0.0.0 if no limitations on multicast source are to be implemented. If you want to establish a source address, set the relevant address.
PORT | 01024 to 65535 (Factory setting: 49326) (Setting 10670 is prohibited.) | Sets the PORT for PGM1 AUDIO RX.
PGM2 AUDIO RX | This is the setting for the PGM2 input.
MCAST ADDR | (Factory setting: 224.1.0.27) | Sets the IP address for PGM2 AUDIO RX.
SOURCE ADDR | (Factory setting: 0.0.0.0) | Set to 0.0.0.0 if no limitations on multicast source are to be implemented. If you want to establish a source address, set the relevant address.
PORT | 01024 to 65535 (Factory setting: 49327) (Setting 10670 is prohibited.) | Sets the PORT for PGM2 AUDIO RX.
SET EXECUTE | - | When you press the [SELECT] button, [NETWORK(SCD RX) SET EXECUTE NO/YES] appears. Select [YES] to apply the configured [NETWORK(SFP+ SCD RX)] information to the unit. If this operation is not performed, the changed [NETWORK(SFP+ SCD RX)] settings will not be applied. In addition, if you exit the menu without performing this operation, the settings will return to their original values.
INCOM1 AUDIO RX | This is the setting for the INCOM1 input.
MCAST ADDR | (Factory setting: 224.1.0.28) | Sets the IP address for INCOM1 AUDIO RX.
SOURCE ADDR | (Factory setting: 0.0.0.0) | Set to 0.0.0.0 if no limitations on multicast source are to be implemented. If you want to establish a source address, set the relevant address.
PORT | 01024 to 65535 (Factory setting: 49328) (Setting 10670 is prohibited.) | Sets the PORT for INCOM1 AUDIO RX.
INCOM2 AUDIO RX | This is the setting for the INCOM2 input.
MCAST ADDR | (Factory setting: 224.1.0.29) | Sets the IP address for INCOM2 AUDIO RX.
SOURCE ADDR | (Factory setting: 0.0.0.0) | Set to 0.0.0.0 if no limitations on multicast source are to be implemented. If you want to establish a source address, set the relevant address.
PORT | 01024 to 65535 (Factory setting: 49329) (Setting 10670 is prohibited.) | Sets the PORT for INCOM2 AUDIO RX.
SET EXECUTE | - | When you press the [SELECT] button, [NETWORK(SCD RX) SET EXECUTE NO/YES] appears. Select [YES] to apply the configured [NETWORK(SFP+ SCD RX)] information to the unit. If this operation is not performed, the changed [NETWORK(SFP+ SCD RX)] settings will not be applied. In addition, if you exit the menu without performing this operation, the settings will return to their original values.

#### NETWORK(1GbE)

This is the selection screen for the NETWORK(1GbE) menu.

Item | Setting value | Setting details
--- | --- | ---
DHCP | OFF, ON (Factory setting: OFF) | Enables/disables DHCP.
IP ADDR | (Factory setting: 192.168.0.52) | Sets the IP address for 1GbE (LAN2).
PORT | (Factory setting: 49330) | Sets the PORT for 1GbE (LAN2).
SUBNETMASK | (Factory setting: 255.255.255.0) | Sets the subnet mask.
DEFAULT GATEWAY | (Factory setting: 192.168.0.1) | Sets the default gateway.
MAC ADDR | Display only | Displays the MAC address.
SET EXECUTE | - | When you press the [SELECT] button, [NETWORK(1GbE) SET EXECUTE NO/YES] appears. Select [YES] to apply the configured [NETWORK(1GbE)] information to the unit. If this operation is not performed, the changed [NETWORK(1GbE)] settings will not be applied. In addition, if you exit the menu without performing this operation, the settings will return to their original values.
DNS | MANUAL, AUTO (Factory setting: MANUAL) | Sets whether the DNS server address is to be acquired automatically (AUTO), or to be input manually (MANUAL). This can be set only from the web screen (AK-NP600).
PRIMARY |  | This can be set only from the web screen (AK-NP600).
SECONDARY |  | This can be set only from the web screen (AK-NP600).
DOMAIN |  | The value allocated by the DHCP server is displayed. (Up to 253 characters, display up to 128 characters) This can be set only from the web screen (AK-NP600).

#### NETWORK(TALLY IN)

This is the selection screen for the NETWORK(TALLY IN) menu.

Item | Setting value | Setting details
--- | --- | ---
INDEX NO | 1 to 65534 (Factory setting: 1) | Sets the INDEX NO set by devices that output TALLY.
PORT | 60000 to 65535 (Factory setting: 62000) | Sets the PORT for TALLY IN.
SET EXECUTE | - | When you press the [SELECT] button, [NETWORK(TALLY IN) SET EXECUTE NO/YES] appears. Select [YES] to apply the configured [NETWORK(TALLY IN)] information to the unit. If this operation is not performed, the changed [NETWORK(TALLY IN)] settings will not be applied. In addition, if you exit the menu without performing this operation, the settings will return to their original values.

NOTE

- The IP address of TALLY IN becomes the setting of the connected IP network.

  Ex.: When input from SFP+ primary

  The main IP ADDR of NETWORK(SFP+ PRM) is enabled.

#### NETWORK(PTP)

This is the selection screen for the NETWORK(PTP) menu.

Item | Setting value | Setting details
--- | --- | ---
DOMAIN | 0 to 127 (Factory setting: 127) | Sets the DOMAIN number.
SET EXECUTE | - | When you press the [SELECT] button, [NETWORK(PTP) SET EXECUTE NO/YES] appears. Select [YES] to apply the configured [NETWORK(PTP)] information to the unit. If this operation is not performed, the changed [NETWORK(PTP)] settings will not be applied. In addition, if you exit the menu without performing this operation, the settings will return to their original values.

#### NETWORK(NMOS)

This is the selection screen for the NETWORK(NMOS) menu.

Item | Setting value | Setting details
--- | --- | ---
NMOS CONTROL | ON, OFF (Factory setting: ON) | Enables/disables the NMOS function.
STATUS | ---- (Factory setting: UNREGISTERED,) | Displays the NMOS operation status, such as RDS connection status. (Display only. Settings cannot be modified.)
PORT(IS-04) | 1024 to 65535 (Factory setting: 50040) | Sets the port number on the camera for IS-04 Node API.
PORT(IS-05) | 1024 to 65535 (Factory setting: 50050) | Sets the port number on the camera for IS-05 Connection API.
RDS IP ADDR | 0.0.0.0 to 255.255.255.255 | Displays the discovered IP address.
RDS PORT | 1 to 65535 | Displays the port number automatically discovered.
LABEL SETTING | AUTO MANUAL | AUTO: The LABEL PREFIX cannot be changed. It is fixed to UCU600_**** ("****" is the last four digits of the MAC ADDR). MANUAL: Text can be set in LABEL PREFIX.
LABEL PREFIX | Maximum 16 characters (alphanumeric characters, spaces, ! # % ( ) + , -. / = [ ] _) (Factory setting: UCU600_**** (“****” is the last four digits of the MAC ADDR)) | Sets the prefix appended which is shared with NMOS resource names on this unit.
DISCOVERY | uniDNS, mDNS (Factory setting: uniDNS) | Sets the method for registry discovery.
SET EXECUTE | - | When the [SELECT] button is pressed, [NETWORK(NMOS) SET EXECUTE NO/YES] is displayed. The [NETWORK(NMOS)] information you set is updated in the unit when you select [YES]. The modified [NETWORK(NMOS)] settings are not updated if you do not perform this procedure. Also, if you close the menu without performing this procedure, the modified content returns to the original settings.

Top of the page