- Top
- Web Screen (AK-NP600)
- Displaying the web screen (AK-NP600)
- View system settings screen [System mode]

# View system settings screen [System mode]

The View system settings screen [System mode] enables you to view the related image format, received image information, etc., when this unit is to use MoIP.

The View system settings screen [System mode] consists of [Main], [TX setting status], [Primary RX status], and [Secondary RX status].

#### Main

Click [Main] in the View system settings screen [System mode].

You can view the basic settings for the unit.

Item | Display description
--- | ---
Format | Displays the CCU format settings.
CCU mode | Displays the settings for the format of the signals output from the CCU.

#### TX setting status

Click [TX setting status] in the View system settings screen [System mode].

You can view the format of the TX signal source.

Item | Display description
--- | ---
Video main format | Displays the settings for the format of images output from the main output line.
Video monitor format | Displays the settings for the format of images output from the monitor.
HD trunk format | Displays the settings for the format of the HD trunk.
Audio | Displays the enable/disable settings for audio output.
Audio format | Displays the settings for audio output format.

#### Primary RX status

Click [Primary RX status] in the View system settings screen [System mode].

This will display the received data information for the SFP+ PRIMARY RX signals.

Item | Display description
--- | ---
Return video format | Detect/Undetected Displays whether return images are being received. Sampling rate Displays the sampling rate of the received return images. Width Displays the horizontal resolution of the received return images. Height Displays the vertical resolution of the received return images.
HD prompter format | Detect/Undetected Displays whether HD prompter RX is being received. Sampling rate Displays the sampling rate of the received HD prompter RX. Width Displays the horizontal resolution of the received HD prompter RX. Height Displays the vertical resolution of the received HD prompter RX.
PGM1 format | Detect/Undetected Displays whether PGM1 audio RX is being received. Sampling rate Displays the sampling rate of the received PGM1 audio RX. Payload type Displays the payload type of the received PGM1 audio RX.
PGM2 format | Detect/Undetected Displays whether PGM2 audio RX is being received. Sampling rate Displays the sampling rate of the received PGM2 audio RX. Payload type Displays the payload type of the received PGM2 audio RX.
INCOM1 format | Detect/Undetected Displays whether INCOM1 audio RX is being received. Sampling rate Displays the sampling rate of the received INCOM1 audio RX. Payload type Displays the payload type of the received INCOM1 audio RX.
INCOM2 format | Detect/Undetected Displays whether INCOM2 audio RX is being received. Sampling rate Displays the sampling rate of the received INCOM2 audio RX. Payload type Displays the payload type of the received INCOM2 audio RX.

#### Secondary RX status

Click [Secondary RX status] in the View system settings screen [System mode].

This will display the received data information for the SFP+ Secondary RX signals.

Item | Display description
--- | ---
Return video format | Detect/Undetected Displays whether return images are being received. Sampling rate Displays the sampling rate of the received return images. Width Displays the horizontal resolution of the received return images. Height Displays the vertical resolution of the received return images.
HD prompter format | Detect/Undetected Displays whether HD prompter RX is being received. Sampling rate Displays the sampling rate of the received HD prompter RX. Width Displays the horizontal resolution of the received HD prompter RX. Height Displays the vertical resolution of the received HD prompter RX.
PGM1 format | Detect/Undetected Displays whether PGM1 audio RX is being received. Sampling rate Displays the sampling rate of the received PGM1 audio RX. Payload type Displays the payload type of the received PGM1 audio RX.
PGM2 format | Detect/Undetected Displays whether PGM2 audio RX is being received. Sampling rate Displays the sampling rate of the received PGM2 audio RX. Payload type Displays the payload type of the received PGM2 audio RX.
INCOM1 format | Detect/Undetected Displays whether INCOM1 audio RX is being received. Sampling rate Displays the sampling rate of the received INCOM1 audio RX. Payload type Displays the payload type of the received INCOM1 audio RX.
INCOM2 format | Detect/Undetected Displays whether INCOM2 audio RX is being received. Sampling rate Displays the sampling rate of the received INCOM2 audio RX. Payload type Displays the payload type of the received INCOM2 audio RX.

Top of the page