- Top
- CCU menu
- OPERATION
- OUT FORMAT(HD)

# OUT FORMAT(HD)

This is the selection screen for the OUT FORMAT (HD) menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
SDI OUT1-4 SDI OUT1 | 3G HD | Set the format of the signals to be output from [1] to [4] of the [UHD/HS/HD SDI OUT] connectors. “Output selection conditions” The settings of [SDI OUT5] and [SDI OUT6] are linked and change together. [SFP+ OUT] is displayed when a MoIP board (AK-NP600) is connected. [SFP+ OUT] follows the [SDI OUT1-4] setting in the same way as [SDI OUT 1/2/3/4]. Output from SFP+ is enabled only when CCU MODE is set to [1080/59.94P], [720/59.94p], [1080/50p], or [720/50p].
SDI OUT1-4 SDI OUT2
SDI OUT1-4 SDI OUT3
SDI OUT1-4 SDI OUT4
SDI OUT1-4 SFP+ OUT
SDI OUT5&6 | 3G HD PsF trueP OVER(3G) | Set the format of the signals to be output from [5] to [7] of the [HD SDI OUT] connectors. The settings of [SDI OUT5] and [SDI OUT6] are linked and change together. When [CCU MODE] is [1080/29.97PsF], [1080/23.98PsF] or [1080/25PsF]: PsF/trueP/OVER(3G) SDI OUT5&6 and SDI OUT7 are set to the same signal. (They cannot be set individually.) When [CCU MODE] is other than [1080/29.97PsF], [1080/23.98PsF], [1080/25PsF]: 3G/HD “Output selection conditions”
SDI OUT7
SDI OUT8 | HD PsF | Set the format of the signals to be output from [8/PM] of the [HD SDI OUT] connector. When [CCU MODE] is [1080/29.97PsF], [1080/23.98PsF] or [1080/25PsF]: PsF (fixed) When [CCU MODE] is other than [1080/29.97PsF], [1080/23.98PsF], [1080/25PsF]: HD (fixed) “Output selection conditions”
SDI OUT8 NORMAL/PM | PM NORMAL | Set the signal to be output from [8/PM] of the [HD SDI OUT] connector. Can only be set to PM when using a MoIP board (AK-NP600). PM : Output the picture monitor images. NORMAL : Output the main line images.
3G SDI | LEVEL-A LEVEL-B | Set the output format for 3G output.

#### Output selection conditions

FORMAT / CCU MODE | SDI | ANALOG
--- | --- | ---
OUT1 | OUT2 | OUT3 | OUT4 | OUT5 | OUT6 | OUT7 | OUT8 | COMPOSITE /PM
HD (59.94)
| 1080 /59.94p | 3G /HD | HD | NORMAL /PM
1080 /29.97PsF | HD | PsF, TrueP, OVER(3G) | PsF | NORMAL /PM
1080 /23.98PsF | HD | PsF, TrueP, OVER(3G) | PsF | NORMAL /PM
1080 /23.98p over 59.94i | HD | HD | NORMAL /PM
1080 /23PsF & over59i | HD | HD | NORMAL /PM
720 /59.94p | HD | HD | NORMAL /PM
HD (50)
| 1080 /50p | 3G /HD | HD | NORMAL /PM
1080 /25psF | HD | PsF, TrueP, OVER(3G) | PsF | NORMAL /PM
720 /50p | HD | HD | NORMAL /PM

#### With AK-NP600 option

FORMAT / CCU MODE | SDI | SFP+
--- | --- | ---
OUT1 | OUT2 | OUT3 | OUT4 | OUT5 | OUT6 | OUT7 | OUT8 | 1 / 2
HD (59.94)
| 1080 /59.94p | 3G /HD | HD | 3G/HD
1080 /23PsF & over59i | HD | HD | no signal
1080 /23.98p over 59.94i | HD | HD | no signal
1080 /29.97PsF | HD | PsF, TrueP, OVER(3G) | PsF | no signal
1080 /23.98PsF | HD | PsF, TrueP, OVER(3G) | PsF | no signal
720 /59.94p | HD | HD | HD
HD (50)
| 1080 /50p | 3G /HD | HD | 3G/HD PM
1080 /25PsF | HD | PsF, TrueP, OVER(3G) | PsF | no signal
720 /50p | HD | HD | HD

Top of the page