- Top
- Web Screen (AK-NP600)
- Displaying the web screen (AK-NP600)
- Notice regarding the Web screen

# Notice regarding the Web screen

#### IP address and subnet mask

Select an IP address for the personal computer within the private address range while ensuring that it is different from the address of the unit. Set the subnet mask to the same address as the unit.

- Unit’s IP address and subnet mask (factory settings)

IP address | 192.168.0.52
Subnet mask | 255.255.255.0

NOTE

- In the factory settings, the variable range for private addresses is between 192.168.0.1 and 192.168.0.255.

#### Personal computer environment required to display the Web screen

For details on the personal computer environment required to display the Web screen, refer to following page.

“Personal computer requirements”

Top of the page