- Top
- CCU menu
- AUDIO
- STBY INTERCOM

# STBY INTERCOM

This is the selection screen for the STBY INTERCOM menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
INPUT LEVEL | -40dB to 0dB to +20dB (1dB Step) | Set the standby intercom input signal level.
OUTPUT LEVEL | -40dB to 0dB to +20dB (1dB Step) | Set the standby intercom output signal level.
CANCEL LEVEL | -20.0dB to +20.0dB *1 (0.5dB Step) | Set the standby intercom I/O cancellation signal level.
STBY INCOM ON/OFF | ON OFF | Set the standby intercom to ON or OFF.

The default setting varies depending on adjustment at the factory.

Top of the page