- Top
- CCU menu
- OPERATION
- MONITOR

# MONITOR

This is the selection screen for the MONITOR menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
R | OFF ON | For the setting details, see the following table. “MONITOR menu setting and operation” ON can be set for [R], [G], and [B] simultaneously. Select one of [R], [G] or [B], and one of [SEQ] or [ENC]. When [SEQ] and [ENC] are set to [ON], [R], [G], and [B] will be set to [OFF]. When [SEQ] and [ENC] are set to [OFF], [R], [G], and [B] will return to their previous configuration.
G | OFF ON
B | OFF ON
SEQ | OFF ON
ENC | OFF ON

#### MONITOR menu setting and operation

The MONITOR menu (R/G/B/SEQ/ENC) operates as follows according to its setting.

MONITOR menu | HDTV | SDTV | Remarks
--- | --- | --- | ---
SDI8/PM | VBS/PM | VBS/PM
R | R | R | R | Output R instead of Y. PBPR and chroma signals OFF.
G | G | G | G | Output G instead of Y. PBPR and chroma signals OFF.
B | B | B | B | Output B instead of Y. PBPR and chroma signals OFF.
SEQ | YPBPR | Y | Y | Chroma signal OFF for VBS output.
ENC | YPBPR | VIDEO | VIDEO | Output normal color images.

Top of the page