- Top
- Web Screen
- Displaying the web screen
- Displaying the web screen using a personal computer

# Displaying the web screen using a personal computer

The procedure is explained here using Windows (Internet Explorer) screens, but it is the same when using the Mac (Safari) screens. (There may be differences in some parts of the screen displays.)

1.Start the web browser of the personal computer.

Use one of the web browsers below depending on the operating system installed in the personal computer.

Installed OS | Web browser
--- | ---
Windows | Internet Explorer
OS X (Mac) | Safari

2.Enter the IP address you configured on the Easy IP Setup Software in the address bar of the web browser.

Example of input

http://registered URL

http://192.168.0.20

If the HTTP port number has been changed from 80, enter [http://<camera IP address>:<port number>] in the address bar.

Ex.: When the port number is set to 8080 :

http://192.168.0.20:8080

When this unit is in a local network, set a proxy server from the web browser ([Tools] - [Internet Options] in the menu bar) to ensure that a proxy server is not used for a local address.

3.Press the [Enter] key.

The web screen appears.

The [Live] screen is displayed initially. You can switch to the [Setup] screen when necessary.

“Switching the [Live] screen or [Setup] screen”

NOTE

- If the personal computer does not have the plug-in viewer software already installed, an installation confirmation message is displayed before the [Live] screen is displayed. In a case like this, follow the on-screen instructions to install the software. [Windows]

“Installing the plug-in viewer software”

- When “User auth.” is set to [On], the user name and password input screen is displayed before the [Live] screen appears.

The default settings for the user name and password are as follows.

User name: admin

Password: 12345

- While the initial settings remain used for the user name and password, a message prompting the user to change the user name and password is displayed after authorization. In order to ensure security, the password for the user name of “admin” must be changed without fail. It is also recommended that the password be changed at regular intervals.

- When an attempt is made to display multiple H.264 images on one personal computer, IP videos may not be displayed depending on the performance of the personal computer concerned. [Windows]

- When an item which is underlined on the screen is clicked, a separate window opens, and an input example is displayed.

- Up to 14 users (consisting of users receiving H.264 images and users receiving JPEG images) can access the unit at the same time. However, depending on the settings for the [Bandwidth control (bit rate)] and [Max bit rate (per client)], the number of users who can access the unit may be limited to less than 14. A message indicating the access limit will appear if the number of users exceeds 14. When [Transmission type] is set to [Multicast port] for [H.264], the second and subsequent users receiving H.264 images will not be counted toward the total access count.

- When “H.264 transmission” is set to [On], H.264 images are displayed. When it is set to [Off], JPEG images will be displayed. JPEG images can be displayed even when [H.264 transmission] is set to [On]. In such cases, however, the maximum frame rate for JPEG images will be 5 fps. [Windows]

- The frame rate for JPEG images may be slower depending on the network environment, performance of your personal computer, subject of the video, and access volume.

<Frame rate for JPEG images>

When [H.264 transmission] is [On]: Maximum 5 fps

When [H.264 transmission] is [Off]: Maximum 30 fps

Top of the page