- Top
- Web Screen
- [Setup] screen
- [User mng.] screen

# [User mng.] screen

The users and personal computers (IP addresses) that can access the unit from personal computers are registered in the [User mng.] screen.

The [User mng.] screen consists of [User auth.] tab and [Host auth.] tab.

#### [User auth.] tab

Click the [User auth.] tab of [User mng.] screen.

Configure the user authorization settings for the personal computers that can access the unit.

Up to 18 users can be registered.

NOTE

- If user authentication fails more than 8 times within a 30-second period from the same IP address (personal computer), access to the unit will be disabled for a certain period.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
User auth. | On Off | Set whether to perform user authorization. On Perform user authentication. Off Do not perform user authentication.
Authentication | Digest or Basic Digest Basic | Specify the method of user authentication to use. The authorization configured here is used for authentication when accessing the web screen. Digest authentication will always be used for connection with the controller. Digest or Basic Use digest authentication or basic authentication. Digest Use digest authentication. Basic Use basic authentication. If you change the [Authentication] setting, close the web browser and perform access again.
User name |  | Enter the user name. Maximum number of characters 1 to 32 half-size characters Invalid characters Full-size and half-size " : ; & \ symbols If you enter a new name for a registered user and click the [Set] button, the user information will be overwritten.
Password Retype password |  | Enter the password. Maximum number of characters 4 to 32 half-size characters Invalid characters Full-size and half-size " &
Access level | 1. Administrator 2. Live only | Select one of the following settings as the user access level. 1. Administrator This access level allows the user to perform all the unit’s operations. 2. Live only This access level enables only [Live] screen to be displayed. The unit cannot be operated or set.
User check |  | You can view registered users by clicking [] for [User check]. A registered user is indicated in the form of “Registered user name [Access level].” (Example: admin[1]) You can delete selected users by clicking the [Delete] button at the right.

#### [Host auth.] tab

Click the [Host auth.] tab of [User mng.] screen.

Configure the host authorization settings that restrict the personal computers (IP addresses) that can access the unit.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
Host auth. | On Off | Set whether to perform host authorization. On Perform host authentication. Off Do not perform host authentication.
IP address |  | The IP address of the personal computer from which access to the unit is allowed is input here. The host name cannot be input as the IP address. When the “IP address/subnet mask length” is input, the personal computers which are allowed to access the camera can be restricted on a subnet by subnet basis. If, for instance, “192.168.0.1/24” has been input and the [1. Administrator] setting has been selected as the [Access level] setting, the personal computers from “192.168.0.1” to “192.168.0.254” will be able to access the camera at the [1. Administrator] access level. When an already registered IP address is input and the [Set] button is clicked, the host information will be overwritten.
Access level | 1. Administrator 2. Live only | Set the host access level. 1. Administrator This access level allows the user to perform all the unit’s operations. 2. Live only This access level enables only [Live] screen to be displayed. The unit cannot be operated or set.
Host check |  | You can view registered host IP addresses by clicking [] for [Host check]. A host is indicated in the form of “Registered IP address [Access level].” (Example: 192.168.0.21 [1]) You can delete selected hosts (IP addresses) by clicking the [Delete] button at the right.

Top of the page