- Top
- CCU menu
- MAINTENANCE
- ANALOG GAIN

# ANALOG GAIN

This is the selection screen for the ANALOG GAIN menu.

Item | Setting value | Setting details
--- | --- | ---
VBS | -50 to +50 | Set the signal level to be output from [VBS OUT] connector.
VBS/PM | -50 to +50 | Set the signal level to be output from [VBS PM OUT] connector.
PROMPT1 | -50 to +50 | Set the ANALOG PROMPT 1 signal level.
PROMPT2 | -50 to +50 | Set the ANALOG PROMPT 2 signal level.

Top of the page