- Top
- CCU menu
- AUDIO
- FORMAT(MOIP)

# FORMAT(MOIP)

This is the selection screen for the FORMAT(MOIP) menu.

Item | Setting value | Setting details
--- | --- | ---
MIC1 TX FORMAT | [1ms/2ch], [1ms/4ch], [1ms/8ch], [0.125ms/2ch], [0.125ms/4ch], [0.125ms/8ch], [0.125ms/16ch], [0.125ms/64ch] | Sets the format for MIC1 output.
MIC2 TX FORMAT | [1ms/2ch], [1ms/4ch], [1ms/8ch], [0.125ms/2ch], [0.125ms/4ch], [0.125ms/8ch], [0.125ms/16ch], [0.125ms/64ch] | Sets the format for MIC2 output.
PGM1 RX FORMAT | [1ms/2ch], [1ms/4ch], [1ms/8ch], [0.125ms/2ch], [0.125ms/4ch], [0.125ms/8ch], [0.125ms/16ch], [0.125ms/64ch] | Sets the format for PGM1 input.
PGM2 RX FORMAT | [1ms/2ch], [1ms/4ch], [1ms/8ch], [0.125ms/2ch], [0.125ms/4ch], [0.125ms/8ch], [0.125ms/16ch], [0.125ms/64ch] | Sets the format for PGM2 input.
INCOM1 TX FORMAT | [1ms/2ch], [1ms/4ch], [1ms/8ch], [0.125ms/2ch], [0.125ms/4ch], [0.125ms/8ch], [0.125ms/16ch], [0.125ms/64ch] | Sets the format for INCOM1 output.
INCOM2 TX FORMAT | [1ms/2ch], [1ms/4ch], [1ms/8ch], [0.125ms/2ch], [0.125ms/4ch], [0.125ms/8ch], [0.125ms/16ch], [0.125ms/64ch] | Sets the format for INCOM2 output.
INCOM1 RX FORMAT | [1ms/2ch], [1ms/4ch], [1ms/8ch], [0.125ms/2ch], [0.125ms/4ch], [0.125ms/8ch], [0.125ms/16ch], [0.125ms/64ch] | Sets the format for INCOM1 input.
INCOM2 RX FORMAT | [1ms/2ch], [1ms/4ch], [1ms/8ch], [0.125ms/2ch], [0.125ms/4ch], [0.125ms/8ch], [0.125ms/16ch], [0.125ms/64ch] | Sets the format for INCOM2 input.

Top of the page