- Top
- Web Screen
- Displaying the web screen
- Notice regarding the Web screen

# Notice regarding the Web screen

#### IP address and subnet mask

Select an IP address for the personal computer within the private address range while ensuring that it is different from the address of the unit. Set the subnet mask to the same address as the unit.

If you need to change the IP address and subnet mask, be sure to ask your dealer to make these changes for you.

- Unit’s IP address and subnet mask (factory settings)

IP address | 192.168.0.20
Subnet mask | 255.255.255.0
Range of private addresses | 192.168.0.0 to 192.168.0.255

#### Personal computer environment required to display the Web screen

For details on the personal computer environment required to display the Web screen, refer to following page.

“Personal computer requirements”

- Some functions on the web setting screen can be used only from a personal computer which is running Windows. (They cannot be used from a personal computer which is running OS X (Mac).)

Functions which can be used by Windows only are indicated using [Windows].

- The "Network Camera View 4S" plug-in viewer software must have already been installed in order to display the unit's IP videos using a personal computer which is running Windows. (This is not required for a personal computer which is running OS X (Mac).)

“Installing the plug-in viewer software”

Top of the page