- Top
- CCU menu
- OPERATION
- SD PHASE

# SD PHASE

This is the selection screen for the SD PHASE menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
SD H COARSE | -30 to 0 to +30 | Make the coarse setting of the H_FINE phase used with GL SD REF.
SD H FINE | -100 to 0 to +100 | Make the fine setting of the H_FINE phase used with GL SD REF.
SD-HD V | 0H ADVANCE 0H_SD_DLAY | Set the vertical phase used with down-convert SD REF. With [1080/59.94i(24P)], this is fixed to [0H]. With [720/59.94p] and [720/50p], this is fixed to [0H].
SCH | -180 to 0 to +180 | Adjust the SCH phase of VBS output.

#### SD signal phase <1080i/59.94 Hz format>

#### SD-HD V item setting: 0H

#### SD-HD V item setting: ADVANCE (90H)

#### SD-HD V item setting: 0H_SD_DLAY (1FRAME-90H DLY)

#### SD signal phase <1080i/50 Hz format>

#### SD-HD V item setting: 0H

#### SD-HD V item setting: ADVANCE (75H)

#### SD-HD V item setting: 0H_SD_DLAY (1FRAME-75H DLY)

#### HD signal phase <1080i/59.94 Hz format>

#### SD-HD V item setting: 0H

#### SD-HD V item setting: ADVANCE (90H)

#### SD-HD V item setting: 0H_SD_DLAY (1FRAME-90H DLY)

#### HD signal phase <1080i/50 Hz format>

#### SD-HD V item setting: 0H

#### SD-HD V item setting: ADVANCE (75H)

#### SD-HD V item setting: 0H_SD_DLAY (1FRAME-75H DLY)

Top of the page