- Top
- Picture monitor (PM)
- Information display
- Status displays

# Status displays

From the IRIS display screen, press the [CHARA] button of the ROP to display the “status display screen”.

However, when the “IRIS LEVEL” setting is “OFF”, the screen will be displayed first if the [CHARA] button of the ROP is pressed when the information is not displayed on the picture monitor.

When the “status display screen” appears, pressing the [CHARA] button of the ROP again displays the status screen.

Pressing the [CHARA] button repeatedly switches display through the status screens in the sequence 1/7 → 2/7 → 3/7 → 4/7 → 5/7 → 6/7 → 7/7 → 1/7 ….

#### Status display screen

A.Camera number

B.System format

C.Scene file number

Not displayed when SCENE FILE is set to OFF.

D.Shutter value

E.CCU format information

F.COLORIMETRY (Y/C conversion coefficient) information

G.Extender information

H.Lens information

I.Zoom position

J.Focus position

K.Optical signal reception status (camera and CCU)

L.ND/CC filter value

The CC filter value is not displayed when AK-UC3300 and AK-PLV100 are connected.

M.Color temperature

N.IRIS F value

O.TALLY INFO

- Set each item to be displayed on the [PM VIEW SETTING] screen that can be accessed by selecting [MAINTENANCE] on the CCU menu.

- The camera format indicates the format of the signal output from the camera.

- Pressing the [CHARA] button of the ROP from the status display screen displays the “status screen”.

- TALLY INFO (L)

Display the R tally in two segments of the upper row and the R, G, or YL tally in two segments of the lower row.

When all R, G, and YL tally signals are ON, the upper row is red, and the left and right segments of the lower row are green and yellow, respectively.

When the R and G tally signals are ON, the upper row is red and the lower row is green.

P.V-LOG information

#### Status displays (page 1 of 7)

Item | Display range | Remarks
--- | --- | ---
HLG MODE | FIX VAR | The HLG mode is displayed here.
SDR MODE | FIX VAR | The SDR mode is displayed here.
HLG B.GAMMA | OFF ON | The status of black gamma when HLG is enabled is displayed here.
HLG KNEE | OFF ON | The status of knee when HLG is enabled is displayed here.
SDR CONV GAIN | –12 –11 –10 –9 –8 –7 –6 –5 0 | The gain value when HDR video is converted to SDR video is displayed here.
SDR CONV POINT | 0 to 100 | The video level to start compression for SDR video is displayed here.
SDR CONV SLOPE | 0 to 127 | The slope to compress video signals is displayed here.

#### Status displays (page 2 of 7)

Item | Display range | Remarks
--- | --- | ---
CAM No. | 1 to 99 | The camera number is displayed here.
CAM FAN MODE | OFF POWERFUL SILENT NORMAL | Indicates the operational mode of the camera fan.
BLACK SHADING | OFF ON | The status of the black shading is displayed here.
WHITE SHADING | OFF ON | The status of the white shading is displayed here.
FLARE | OFF ON | The status of the FLARE is displayed here.
GAMMA | OFF ON | The status of the gamma correction is displayed here.
BLACK GAMMA | OFF ON | The status of the black gamma is displayed here. This function changes the amplification rate of the video signals in the low-brightness areas.
KNEE | OFF ON | The status of the knee function is displayed here. This function attenuates that part of the video signal that exceeds the prescribed level (knee point) to minimize saturation.
WHITE CLIP | OFF ON | The status of the white clip function is displayed here.
DRS SW | OFF ON | The status of the DRS SW is displayed here.
MATRIX | OFF ON | The status of the matrix function is displayed here. This function compensates the saturation and hue.
SHUTTER | Setting values on camera | The speed of the electronic shutter is displayed here. For the setting values, refer to the Operating Instructions for the camera.

#### Status displays (page 3 of 7)

When AK-PLV100 is connected, if the setting on AK-PLV100 of [MODE] in [SWITCH MODE] → [GAIN SETTING] is [ISO], [M.GAIN] becomes [ISO SELECT] and [M.GAIN VAR] becomes [ISO].

When [MODE] is [dB] | When [MODE] is [ISO]

Item | Display range | Remarks
--- | --- | ---
GAMMA MODE | HD FILMLIKE1 FILMLIKE2 FILMLIKE3 FILM REC VIDEO REC | The selected gamma type is displayed here.
M.GAIN ISO SELECT | -6dB to 36dB NATIVE/800/2500 | The gain increase value is displayed here. The ISO operation set on AK-PLV100 is displayed here.
M.GAIN VAR ISO | -6dB to 36dB 200 to 25600 | The gain offset value is displayed here. The ISO value set on AK-PLV100 is displayed here.
UHD DETAIL | OFF ON | The status of the UHD DETAIL is displayed here.
UHD SKIN TONE DETAIL | OFF ON | Indicates the status of the SKIN TONE DETAIL function. This function minimizes the detail components applied to skin tone.
HD DETAIL | OFF ON | The status of the HD DETAIL is displayed here.
HD SKIN TONE DETAIL | OFF ON | Indicates the status of the SKIN TONE DETAIL function. This function minimizes the detail components applied to skin tone.
ND FILTER | **** | The names of the ND filters are displayed here. Indicates the names (4 letters each) corresponding to ND filters 1 to 5. The names configured in the CCU screen appear. This will be ND filters 1 to 4 when AK-UC3300 and AK-PLV100 are connected.
CC FILTER | **** | The names of the CC filters are displayed here. Indicates the names (5 letters each) corresponding to CC filters A to E. The names configured in the CCU screen appear. This is not displayed when AK-UC3300 and AK-PLV100 are connected.
LENS EXTENDER | 1.0 2.0 | The magnification of the lens extender is displayed here.
AUTO IRIS | OFF ON | The status of the auto IRIS function is displayed here.
SCENE FILE | OFF --- 1 to 8 | The selected scene file is displayed here.

#### Status displays (page 4 of 7)

Item | Display range | Remarks
--- | --- | ---
ASU REF | FACTORY USER1 USER2 USER3 REF1 REF2 REF3 | The reference file used during auto setup is displayed here. This is not displayed when AK-PLV100 is connected.
ASU MODE | OUT FULL OUT EASY | The auto setup mode is displayed here. This is not displayed when AK-PLV100 is connected.
DOWNCONVERT MODE | SC SQ LB LINK | The downconversion mode is displayed here. The displayed abbreviations represent the following. SC: SIDECUT SQ: SQUEEZE LB: LETTERBOX LINK: LINK
UPCONVERT MODE | SC SQ LB LINK | The upconversion mode is displayed here. The displayed abbreviations represent the following. SC: SIDECUT SQ: SQUEEZE LB: LETTERBOX LINK: LINK
RETURN1 | RET1 RET2 RET3 RET4 VBS | The statuses of the input format allocations for SDI return signals 1 to 4 are displayed here.
RETURN2
RETURN3
RETURN4

#### Status displays (page 5 of 7)

Item | Display range | Remarks
--- | --- | ---
SDI OUTPUT1 | UHD 3G HD UHD_HDR HD_HDR HD_SDR | Output formats of SDI OUT1 through SDI OUT4 are displayed here.
SDI OUTPUT2
SDI OUTPUT3
SDI OUTPUT4
SDI OUTPUT5 | UHD 3G HD_1080i HD_1080p HD_720p UHD_HDR 3G_HDR HD_HDR_1080i HD_HDR_1080p HD_SDR_1080i HD_HDR_720p PsF trueP OVER(3G) PsF_SDR trueP_SDR OVER(3G)_SDR PsF_HDR trueP_HDR OVER(3G)_HDR | Output formats of SDI OUT5 through SDI OUT7 are displayed here.
SDI OUTPUT6
SDI OUTPUT7
SDI OUTPUT8 | HD_1080i HD_1080p HD_720p HD_HDR_1080i HD_HDR_1080p HD_SDR_1080i HD_HDR_720p PsF PsF_SDR PsF_HDR | Output format of SDI OUT8 is displayed here.
SDI OUTPUT8 NORMAL / PM | PM NORMAL | The signal to be output from SDI OUT8 is displayed here.
3G SDI | LEVEL-A LEVEL-B | The output format during 3G output is displayed here.
UHD OUTPUT FORMAT | INTERLEAVE SQUARE | The format (INTERLEAVE or SQUARE) of the UHD signals output from SDI OUT1 to SDI OUT4 is displayed here.
HDR COLORIMETRY | BT.709 BT.2020 | The Y/C conversion coefficient is displayed here.

#### Status displays (page 6 of 7)

Item | Display range | Remarks
--- | --- | ---
HD TRUNK/TICO | HD TRUNK TICO | The signal to be output from the [HD TRUNK OUT] connector is displayed here.
COMPOSITE | PM NORMAL | The signal to be output from the [VBS PM OUT] connector is displayed here.

#### Status displays (page 7 of 7)

Item | Display range | Remarks
--- | --- | ---
BUTTON ASSIGN USER1 | NONE CHARA BARS CLEAN | The function assigned to the [USER1] button is displayed here.
BUTTON ASSIGN USER2 | NONE CHARA MENU/USER1 LOCK BARS CLEAN | The function assigned to the [USER2] button is displayed here.
ROP SW | FRONT ONLY REAR ONLY SWITCH SELECT | This displays the operating status (front/rear) of the [ROP] connectors.
HOURS CCU | ******H | Cumulative CCU operating time is displayed here.
CABLE OPEN | (Off) | This item flashes when the optical fiber multi cable is not connected.
CABLE SHORT | (Off) | This item flashes when the optical fiber multi cable is short-circuited.
CAM RECEIVE LEVEL | ■■■■■ | The level of the optical signals received by the camera is displayed in 5 gradations.
CCU RECEIVE LEVEL | ■■■■■ | The level of the optical signals received by the unit is displayed in 5 gradations.
VERSION | - - - | The unit's software version is displayed here.

Top of the page