- Top
- CCU menu
- MAINTENANCE
- AUX

# AUX

This is the selection screen for the AUX menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
FUNCTION | WFM_TYPE-A+SD_ASPECT WFM_TYPE-B+SD_ASPECT AUDIO GAIN+SD_ASPECT | Switch the function of the [AUX] connector. WFM_TYPE-A+SD_ASPECT / WFM_TYPE-B+SD_ASPECT Waveform monitor control output and down-conversion input AUDIO GAIN+SD_ASPECT Camera's MIC gain control output and down-conversion input “Down-conversion mode settings” “AUDIO GAIN settings”

#### Selecting connected waveform monitors

Configure the type of waveform monitor (WFM) to connect to the [AUX] connector as follows.

Setting value | Control mode
--- | ---
TYPE-A | Coded Mode
TYPE-B | Direct Mode

- There are two types of waveform monitor (WFM) you can connect.

- You can recall presets for the waveform monitor in the [MONITOR] menu.

Waveform monitor presets must be configured on the waveform monitor beforehand.

Depending on the model, connection of the waveform monitor to the unit may require cable connections other than those described.

#### Relationship between the MONITOR menu and waveform monitor preset numbers

By using the preset function of the waveform monitor, you can load the waveform monitor's waveform display settings.

MONITOR menu setting | Preset setting numbers of waveform monitor
--- | ---
R | Preset1
B | Preset2
G | Preset3
R+B+G | Preset4
R+B
R+G
B+G
SEQ | Preset5
ENC | Preset6

- For details on the controls that correspond to the preset numbers set on the waveform monitor, consult your dealer.

Top of the page