- Top
- CCU menu
- OPERATION
- SETTING(1/2)

# SETTING(1/2)

This is the selection screen for the SETTING(1/2) menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
COMPOSITE/PM | PM NORMAL | Set the signal to be output from [VBS PM OUT] connector. PM : Output the picture monitor images. NORMAL : Output the main line images. When [SDI OUT8] is set to [NORMAL] in the [OUTPUT FORMAT] menu, this will be fixed at [PM] to maintain the [SDI OUT8] or [COMPOSITE/PM] output picture monitor display.
ANALOG PROMPT | 1-OUT 2-IN | Set input/output for the [ANALOG PROMPT1 IN] and [ANALOG PROMPT2 IN/OUT] connectors. When [1-OUT] is selected, the signal input to the [ANALOG PROMPT1 IN] connector becomes the loop-through output. Apply termination on the connected device.
RETURN FS | ON OFF | Set the delay mode for the HD return signals.
TRUNK1 | RS422 RS232C | Set the TRUNK1 line send/receive format of the [TRUNK] connector.
TRUNK2 | Set the TRUNK2 line send/receive format of the [TRUNK] connector.
MONO SW | ON OFF | Set CCU output video to monochrome.
HD BAR SELECT | STD SMPTE ARIB EIAJ SPLIT | Set the color bar signal for output with the HD signal.
HD BAR LPF | OFF 3TAP 5TAP 7TAP 9TAP | Set the filter to be applied to the color bar signal output with the HD signal.
HD BAR USER1 | 75%WHITE 100%WHITE +I_SIGNAL -I_SIGNAL | Set user selection 1 for when [ARIB] has been selected as the [HD BAR SELECT] setting.
HD BAR USER2 | 0%BLACK +Q_SIGNAL | Set user selection 2 for when [ARIB] has been selected as the [HD BAR SELECT] setting.

Top of the page