- Top
- CCU menu
- OPERATION
- SELECT RETURN

# SELECT RETURN

This is the selection screen for the SELECT RETURN menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
SELECT RETURN1 | RET1 RET2 RET3 RET4 VBS | Set the input assignment of the return signals. Can only be set to RET1 when SFP+ is selected.
SELECT RETURN2 | RET1 RET2 RET3 RET4 VBS
SELECT RETURN3 | RET1 RET2 RET3 RET4 VBS
SELECT RETURN4 | RET1 RET2 RET3 RET4 VBS

Top of the page