- Top
- Reference
- Connector pin assignment table
- Rear panel

# Rear panel

#### [AUX] connector

JAY-15S-1A3F(LF)(SN) (J.S.T. Mfg. Co., Ltd.)

Pin No. | Function | Specifications | Remarks
--- | --- | --- | ---
1 | TALLY YL OUT | Open collector output | “Example of tally and alarm output connections”
2 | P6 | See remarks | When [AUX] > [FUNCTION] is set to [WFM_TYPE-A+SD_ASPECT] or [WFM_TYPE-B+SD_ASPECT] in the [MAINTENANCE] menu: Waveform monitor preset setting bit output Open collector output When [AUX] > [FUNCTION] is set to [AUDIO GAIN+SD_ASPECT] in the [MAINTENANCE] menu: Camera microphone gain setting bit input Photo-coupler input
3 | P5
4 | P4
5 | P3
6 | P2
7 | P1
8 | GND | Ground |
9 | MODE2 | Photo-coupler input | “Down-conversion mode settings” “Example of mode input connections”
10 | MODE1 | Photo-coupler input
11 | GND | Ground |
12 | ALARM | Open collector output | “Example of tally and alarm output connections”
13 | TALLY R OUT | Open collector output | “Example of tally and alarm output connections”
14 | TALLY G OUT | Open collector output | “Example of tally and alarm output connections”
15 | GND | Ground |

#### Down-conversion mode settings

Down-conversion mode | MODE1 | MODE2
--- | --- | ---
Local | Open | Open
Letter box | Shorted | Open
Squeeze | Open | Shorted
Side panel | Shorted | Shorted

Shorted: Shorted with pin 8 (GND)

#### Preset settings of waveform monitor

TYPE-A | AUX connector output
--- | ---
P6 | P5 | P4 | P3 | P2 | P1
PRESET1 | Shorted | Shorted | Shorted | Shorted | Shorted | Open
PRESET2 | Shorted | Shorted | Shorted | Shorted | Open | Shorted
PRESET3 | Shorted | Shorted | Shorted | Shorted | Open | Open
PRESET4 | Shorted | Shorted | Shorted | Open | Shorted | Shorted
PRESET5 | Shorted | Shorted | Shorted | Open | Shorted | Open
PRESET6 | Shorted | Shorted | Shorted | Open | Open | Shorted

TYPE-B | AUX connector output
--- | ---
P6 | P5 | P4 | P3 | P2 | P1
PRESET1 | Open | Open | Open | Open | Open | Shorted
PRESET2 | Open | Open | Open | Open | Shorted | Open
PRESET3 | Open | Open | Open | Shorted | Open | Open
PRESET4 | Open | Open | Shorted | Open | Open | Open
PRESET5 | Open | Shorted | Open | Open | Open | Open
PRESET6 | Shorted | Open | Open | Open | Open | Open

Shorted: Shorted with pin 8 (GND)

#### AUDIO GAIN settings

You can control camera microphone gain from an external device.

Gain control setting | P1 | P2
--- | --- | ---
Disabled | Open | Open
MIC1 enabled | Shorted | Open
MIC2 enabled | Open | Shorted
MIC1 and MIC2 enabled | Shorted | Shorted

Camera microphone gain setting | Total gain | P3 | P4 | P5
--- | --- | --- | --- | ---
MIC GAIN | AMP
60 | 0 | 60 dB | Open | Open | Open
40 | 10 | 50 dB | Shorted | Open | Open
40 | 0 | 40 dB | Open | Shorted | Open
20 | 10 | 30 dB | Shorted | Shorted | Open
20 | 0 | 20 dB | Open | Open | Shorted

Shorted: Shorted with pin 8 (GND)

#### Example of mode input connections

#### Example of tally and alarm output connections

#### [TRUNK] connector

JEY-9S-1A3F (LF)(SN) (J.S.T. Mfg. Co., Ltd.)

Pin No. | Function | Flow of signal | Remarks
--- | --- | --- | ---
1 | TRUNK1_TX (C) | CAM → CCU | RS-422 / RS-232C Selected using a menu Connect to the (C) side during RS-232C connections. The (H) is open.
2 | TRUNK1_TX (H) | CAM → CCU
3 | TRUNK1_RX (H) | CCU → CAM
4 | TRUNK1_RX (C) | CCU → CAM
5 | GND |
6 | TRUNK2_TX (C) | CAM → CCU
7 | TRUNK2_TX (H) | CAM → CCU
8 | TRUNK2_RX (H) | CCU → CAM
9 | TRUNK2_RX (C) | CCU → CAM

#### [COMMUNICATION] connector

JBY-25S-1A3F(LF)(SN) (J.S.T. Mfg. Co., Ltd.)

Pin No. | Function | Flow of signal | Remarks
--- | --- | --- | ---
1 | INCOM ENG OUT (H) | CCU→SYSTEM | 0 dBm, 600 Ω (4 W) / 1 V [p-p], 200 Ω (RTS) 4 W/RTS/CLRCOM Selected using a menu
2 | INCOM ENG OUT (C) | CCU→SYSTEM
3 | INCOM ENG (GND) |
4 | INCOM ENG IN (H) | SYSTEM→CCU
5 | INCOM ENG IN (C) | SYSTEM→CCU
6 | PGM IN (H) | SYSTEM→CCU | 0 dBm/-20 dBm, 600 Ω Selected using a menu
7 | PGM IN (C) | SYSTEM→CCU
8 | PGM IN (GND) |
9 | GND |  |
10 | NC |  |
11 | R TALLY IN (H) | SYSTEM→CCU | ON: Short/TTL(H)/24 V “Example of tally input connections” OFF: Open/TTL(L)/0 V
12 | R TALLY IN (C) | SYSTEM→CCU
13 | GND |  |
14 | INCOM PROD OUT (H) | CCU→SYSTEM | 0 dBm, 600 Ω (4 W) / 1 V [p-p], 200 Ω (RTS) 4 W/RTS/CLRCOM Selected using a menu
15 | INCOM PROD OUT (C) | CCU→SYSTEM
16 | INCOM PROD (GND) |
17 | INCOM PROD IN (H) | SYSTEM→CCU
18 | INCOM PROD IN (C) | SYSTEM→CCU
19 | PGM2 IN (H) | SYSTEM→CCU | 0 dBm/-20 dBm, 600 Ω Selected using a menu
20 | PGM2 IN (C) | SYSTEM→CCU
21 | PGM2 IN (GND) |
22 | YL TALLY IN (H) | SYSTEM→CCU | ON: Short/TTL(H)/24 V “Example of tally input connections” OFF: Open/TTL(L)/0 V
23 | YL TALLY IN (C) | SYSTEM→CCU
24 | G TALLY IN (H) | SYSTEM→CCU
25 | G TALLY IN (C) | SYSTEM→CCU

#### Example of tally input connections

Equivalent circuit

#### [ROP] connector

HR10G-10R-10SC (71) (Hirose Electric Co., Ltd.)

Pin No. | Function | Flow of signal
--- | --- | ---
1 | ROP CONT (H) | CCU→ROP
2 | ROP CONT (C) | CCU→ROP
3 | ROP DATA (H) | ROP→CCU
4 | ROP DATA (C) | ROP→CCU
5 | NC |
6 | NC |
7 | NC |
8 | NC |
9 | +16 V OUT | CCU→ROP
10 | GND |

- Connector of cable

HR10A-10P-10P (73)

#### [MSU] connector

HR10G-10R-10SC (71) (Hirose Electric Co., Ltd.)

Pin No. | Function | Flow of signal
--- | --- | ---
1 | MSU CONT (H) | CCU→MSU
2 | MSU CONT (C) | CCU→MSU
3 | MSU DATA (H) | MSU→CCU
4 | MSU DATA (C) | MSU→CCU
5 | TALLY R | CCU→MSU
6 | TALLY G | CCU→MSU
7 | HEAD POWER | CCU→MSU
8 | ALARM 1 | CCU→MSU
9 | ALARM 0 | CCU→MSU
10 | GND |

- Connector of cable

HR10A-10P-10P (73)

#### [MIC1] and [MIC2] connectors

HA16RV-3PG(76) (Hirose Electric Co., Ltd.)

Pin No. | Function | Flow of signal | Remarks
--- | --- | --- | ---
1 | SHIELD |  | 0 dBm, 600 Ω
2 | HOT | CCU→SYSTEM
3 | COLD | CCU→SYSTEM

- When connecting to an unbalanced input terminal of an external device, connect to it as shown in the diagram below.

- Some commercially available conversion connectors and conversion cables have pin 3 shorted to pin 1.

Using such a conversion connector or conversion cable will cause a failure.

#### [CAMERA] connector

AK-UCU600: OPS2404-PR (Tajimi Electronics Co., Ltd.)

AK-UCU600S: FXW.3K.93C.TLM (LEMO)

Pin No. | Function | Flow of signal
--- | --- | ---
1 | Optical fiber | CAM → CCU
2 | Optical fiber | CCU → CAM
3 | Control line | CCU←→CAM
4 | Control line | CCU←→CAM
5 | AC 240 V | CCU → CAM
6 | AC 240 V | CCU → CAM

Top of the page