- Top
- Specifications

# Specifications

Power supply | AK-UCU600P/AK-UCU600PS : 100 V - 120 V AC (), 50 Hz/60 Hz AK-UCU600E/AK-UCU600ES : 100 V - 240 V AC (), 50 Hz/60 Hz
Power consumption | 500 W (Without camera connected: 90 W)
Capacity for supplying power to a camera | 240 V AC (), 1.46 A , 50 Hz/60 Hz

indicates safety information.

Operating temperature | 0 °C to 40 °C (32 °F to 104 °F)
Humidity | 10% to 90% (no condensation)
Dimensions (Width×Height×Depth) | 424 mm × 88 mm × 401 mm (16-5/8 inches × 3-7/16 inches × 15-13/16 inches) (excluding protrusions)
Weight | Approx. 8.9 kg (19.6 lb)
Video output | 3G/HD-SDI 5 lines (embedded audio is supported only for HD signals)
12G/6G/3G/HD-SDI 2 lines
HD-SDI 1 line (shared with picture monitor output*2)
Analog composite 2 lines (1 line shared with picture monitor output*2)
HD TRUNK/TICO output | When HD TRUNK: HD-SDI (Supported format: 1080/59i or 1080/50i), 3G/HD-SDI 1 line
Return input | 3G-HD/HD/SD-SDI 4 lines (RET1 input has active-through output)
Analog composite 1 line
Prompter input | HD-SDI 1 line (with active-through output)
Analog composite 2 lines (through output of 1 and input of 2 share the connector*2) It is not terminated when the unit is turned OFF. No through output.
Reference input | BB (black burst) / tri-level*1 1 line (automatic termination, connect to upper connector; BB signal and tri-level signal automatically recognized, with loop-through output)
Microphone output | 0 dBm/600 Ω 2 lines (XLR, 3-pin, male)
Communication | Intercom input/output (ENG / PROD, 0 dBm, 600 Ω (4 W) / 1 V [p-p], 200 Ω (RTS), 4 W / RTS / CLRCOM) 2 lines*2
PGM input (0 dBm/600 Ω) 2 lines
Tally input (red, green, yellow) 1 input each
AUX | WFM control 6-bit (open collector output, terminal shared with camera microphone gain setting*2)
Camera microphone gain setting input 5-bit (photo-coupler input, terminal shared with WFM control*2)
Down-conversion system setting input 2-bit (photo-coupler input)
TRUNK | RS-422 / RS-232C 2 lines*2
FRONT ROP | RS-422 1 line, 16 V DC output (only one of this and REAR ROP can be selected at one time via the menu or the [ROP FRONT/REAR] selection switch on the front panel)
REAR ROP | RS-422 1 line, 16 V DC output (only one of this and FRONT ROP can be selected at one time via the menu or the [ROP FRONT/REAR] selection switch on the front panel)
MSU | RS-422 1 line, GPI for control
LAN TRUNK | LAN connection with camera side via an optical cable*3 1 line, 100BASE-TX, 1000BASE-T
LAN | Personal computer connection for distribution via the Web*3 1 line, 10BASE-T, 100BASE-TX (use a crossover cable when connecting directly with a personal computer)

The BB (black burst) signal and tri-level sync signal of the reference input are recognized automatically.

Depending on the setting, only one of them can be selected at one time.

IP video is cannot be transmitted when [CCU MODE] is set to [2160/23.98p], [2160/23.98psf], [1080/23.98p], or [1080/23.98psF].

The symbols on this product (including the accessories) represent the following:

AC Power on Power off

NOTE

- For details on the maximum lengths of connection cables, consult your dealer.

Inrush current, measured according to European standard EN55103-1, on initial switch-on: 3 A, after a supply interruption of 5 s: 80 A

Top of the page