- Top
- CCU menu
- MAINTENANCE
- ND/CC NAME(2/2)

# ND/CC NAME(2/2)

This is the selection screen for the ND/CC NAME(2/2) menu.

Item | Setting value | Setting details
--- | --- | ---
CC FILTER_1 NAME | 5 characters (Factory setting: A) | Set the name (maximum 5 characters) of CC filter 1 (3200K). The name set here is displayed in the status display (STATUS2). Characters which can be used: Alphanumeric characters, spaces, ! # % & ' ( ) * + , - . / : ; < = > ? [ ] _ ~
CC FILTER_2 NAME | 5 characters (Factory setting: B) | Set the name (maximum 5 characters) of CC filter 2 (4300K). The name set here is displayed in the status display (STATUS2). Characters which can be used: Alphanumeric characters, spaces, ! # % & ' ( ) * + , - . / : ; < = > ? [ ] _ ~
CC FILTER_3 NAME | 5 characters (Factory setting: C) | Set the name (maximum 5 characters) of CC filter 3 (6300K). The name set here is displayed in the status display (STATUS2). Characters which can be used: Alphanumeric characters, spaces, ! # % & ' ( ) * + , - . / : ; < = > ? [ ] _ ~
CC FILTER_4 NAME | 5 characters (Factory setting: D) | Set the name (maximum 5 characters) of CC filter 4 (CROSS). The name set here is displayed in the status display (STATUS2). Characters which can be used: Alphanumeric characters, spaces, ! # % & ' ( ) * + , - . / : ; < = > ? [ ] _ ~
CC FILTER_5 NAME | 5 characters (Factory setting: E) | Set the name (maximum 5 characters) of CC filter 5 (DF0). The name set here is displayed in the status display (STATUS2). Characters which can be used: Alphanumeric characters, spaces, ! # % & ' ( ) * + , - . / : ; < = > ? [ ] _ ~

NOTE

When AK-UC3300 and AK-PLV100 are connected, "ND/CC NAME(2/2)" is not displayed.

Top of the page