- Top
- CCU menu
- UHD SETTING
- HD DETAIL(1/2)

# HD DETAIL(1/2)

This is the selection screen for the HD DETAIL(1/2) menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
DETAIL | OFF ON | Enable/disable the detail function.
MASTER DETAIL | -31 to 0 to 31 | Set the master detail.
DETAIL LEVEL H | 00 to 15 to 63 | Set the horizontal detail correction level.
DETAIL LEVEL V | 00 to 15 to 63 | Set the vertical detail correction level.
PEAK FREQUENCY | 12.4 / 12.5 / 12.7 / 12.9 / 13.0 / 13.3 / 13.6 / 13.9 / 14.2 / 14.6 / 15.0 / 15.5 / 16.1 / 16.7 / 17.3 / 18.3 / 18.6 / 18.8 / 19.0 / 19.2 / 19.5 / 19.9 / 20.3 / 20.9 / 21.5 / 22.4 / 23.6 / 25.4 / 28.6 / 37.1 | Set the peak frequency of the horizontal detail.
V DETAIL FREQUENCY | 00 to 10 to 31 | Set the vertical detail frequency.
CRISP | 00 to 10 to 63 | Set the noise elimination level for the detail signals.
DETAIL GAIN（+） | -31 to 0 to +31 | Increase (+) the detail level.
DETAIL GAIN（-） | -31 to 0 to +31 | Decrease (-) the detail level.
DETAIL CLIP（+） | 00 to +63 | Adjust detail clipping to minimize any roughness that results from excessive detail application.
DETAIL CLIP（-） | 00 to +63 | This limits the length of the undershoot portion of the detail edge component.
DETAIL SOURCE | (G+R)/2 (G+B)/2 (2G+B+R)/4 (3G+R)/4 R G | Set the RGB signal component ratio used for detail creation.
KNEE APERTURE LEVEL | 00 to 39 | Adjust the knee aperture level. For HDR format, this is fixed at [5].
DETAIL KNEE | 00 to 15 | Adjust the knee detail component.

Top of the page