- Top
- CCU menu
- MAINTENANCE
- ND/CC NAME(1/2)

# ND/CC NAME(1/2)

This is the selection screen for the ND/CC NAME(1/2) menu.

Item | Setting value | Setting details
--- | --- | ---
ND FILTER_1 NAME | 5 characters (Factory setting: 1) | Set the name (maximum 5 characters) of ND filter 1 (CAP). The name set here is displayed in the status display (STATUS2). Characters which can be used: Alphanumeric characters, spaces, ! # % & ' ( ) * + , - . / : ; < = > ? [ ] _ ~
ND FILTER_2 NAME | 5 characters (Factory setting: 2) | Set the name (maximum 5 characters) of ND filter 2 (CLEAR). The name set here is displayed in the status display (STATUS2). Characters which can be used: Alphanumeric characters, spaces, ! # % & ' ( ) * + , - . / : ; < = > ? [ ] _ ~
ND FILTER_3 NAME | 5 characters (Factory setting: 3) | Set the name (maximum 5 characters) of ND filter 3 (1/4). The name set here is displayed in the status display (STATUS2). Characters which can be used: Alphanumeric characters, spaces, ! # % & ' ( ) * + , - . / : ; < = > ? [ ] _ ~
ND FILTER_4 NAME | 5 characters (Factory setting: 4) | Set the name (maximum 5 characters) of ND filter 4 (1/16). The name set here is displayed in the status display (STATUS2). Characters which can be used: Alphanumeric characters, spaces, ! # % & ' ( ) * + , - . / : ; < = > ? [ ] _ ~
ND FILTER_5 NAME | 5 characters (Factory setting: 5) | Set the name (maximum 5 characters) of ND filter 5 (1/64). The name set here is displayed in the status display (STATUS2). Characters which can be used: Alphanumeric characters, spaces, ! # % & ' ( ) * + , - . / : ; < = > ? [ ] _ ~

NOTE

When AK-UC3300 and AK-PLV100 are connected, the display for "ND/CC NAME" changes to "ND NAME" and [ND FILTER 5 NAME] is not displayed.

Top of the page