- Top
- Parts and their functions
- Front panel 3

# Front panel 3

1 | [MENU] button | When you hold down the [MENU] button, the menu screen is displayed on the picture monitor and the [MENU] button lights. If you hold down the [MENU] button while the menu is displayed, the menu closes and the [MENU] button turns off. “Menu operations”
2 | [SELECT] dial | This jog dial is for menu screen operations. When the [SELECT] dial is turned clockwise, the cursor moves down; conversely, when it is turned counterclockwise, the cursor moves up. Press the [SELECT] dial to select the menu items. “Menu operations”
3 | [USER1] and [USER2] buttons | These buttons are used for assigning functions. Function assignments are selected using [SETUP] in the CCU menu. The following functions are pre-assigned at the factory. [USER1] button: CHARA [USER2] button: LOCK “SETUP”
4 | [ROP FRONT/REAR] selector switch | This switch switches between the [ROP] connectors on the front and rear panels. This is enabled when [MAINTENANCE] > [SETUP] > [ROP SW] is set to [SWITCH SELECT] in the CCU menu. “ROP SW”
5 | [ROP] connector (front) | This connector is for connecting a ROP (sold separately).
6 | Memory card slot | Insert a memory card (sold separately). A memory card can be used to set this unit. “SD CARD”
7 | Memory card access lamp | This is lit while the memory card is being accessed.

Top of the page