- Top
- CCU menu
- OPERATION
- SETTING(2/2)

# SETTING(2/2)

This is the selection screen for the SETTING(2/2) menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
DOWN CONVERT | SC SQ LB LINK | Set the down-convert system. “Down-conversion mode settings”
UP CONVERT | SC SQ LB LINK | Set the up-convert system.
C/B SETUP*1 | OFF COMPST SD_SDI BOTH | Set the SD signal output for use with color bar output. This is only displayed when the format is 59.94 Hz.

AK-UCU600P/600PS

Top of the page