- Top
- Picture monitor (PM)
- Information display
- Operation displays

# Operation displays

The operation displays appear at the bottom of the screen for approx. 4 seconds when any of the following operations have been performed with the operation panel of the ROP.

- Master gain change

- Electronic shutter change

- Lens extender change

- Scene file change

- REF LOAD is changed

- FILTER is changed

The display time can be changed from [MAINTENANCE] menu > [PM OPERATION STATUS] > [STATUS DISP TIME].

Item | Display range | Remarks
--- | --- | ---
MASTER GAIN | Setting values on camera | The master gain value is displayed here. For the setting values, refer to the Operating Instructions for the camera.
SHUTTER | Setting values on camera | The speed of the electronic shutter is displayed here. For the setting values, refer to the Operating Instructions for the camera.
LENS EXT | 1.0 2.0 | The magnification of the lens extender is displayed here. When the magnification of the lens extender is set to 2x, [2.0] is displayed. Otherwise, [1.0] is displayed.
SCENE FILE | OFF 1 to 8 | This indicates the scene file name.
REF LOAD | FACTORY USER1 to USER3 REF1 to 3 | This indicates the reference file that was loaded via reference call recalling.
FILTER | **** (ND/CC filter name) | The names of the ND filter/CC filters are displayed here.

Top of the page