- Top
- CCU menu
- OPERATION
- OUT FORMAT(HD_HDR)

# OUT FORMAT(HD_HDR)

This is the selection screen for the OUT FORMAT(HD_HDR) menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
SDI OUT1-4 SDI OUT1 | 3G_HDR HD_HDR HD_SDR | Set the format of the signals to be output from [1] to [4] of the [UHD/HS/HD SDI OUT] connectors. The content selected in SDI OUT1-4 is displayed for the items of SDI OUT1-4. “Output selection conditions” [SFP+ OUT] is displayed when a MoIP board (AK-NP600) is connected. [SFP+ OUT] follows the [SDI OUT1-4] setting in the same way as [SDI OUT 1/2/3/4].
SDI OUT1-4 SDI OUT2
SDI OUT1-4 SDI OUT3
SDI OUT1-4 SDI OUT4
SDI OUT1-4 SFP+ OUT
SDI OUT5&6 | 3G_HDR 3G_SDR HD_HDR HD_SDR PsF_HDR TrueP_HDR OVER(3G)_HDR PsF_SDR TrueP_SDR OVER(3G)_SDR | Set the format of the signals to be output from [5] to [7] of the [HD SDI OUT] connectors. The settings of [SDI OUT5] and [SDI OUT6] are linked and change together. When [CCU MODE] is [1080/29.97PsF], [1080/23.98PsF] or [1080/25PsF]: PsF_HDR/PsF_SDR/TrueP_HDR/TrueP_SDR/OVER(3G)_HDR/OVER(3G)_SDR With PsF/TrueP/OVER(3G), the settings made for SDI OUT5&6 are reflected in SDI OUT7, and only switching between HDR/SDR is possible in SDI OUT7. When [CCU MODE] is other than [1080/29.97PsF], [1080/23.98PsF], [1080/25PsF]: 3G_HDR/3G_SDR/HD_HDR/HD_SDR “Output selection conditions”
SDI OUT7
SDI OUT8 | HD_HDR HD_SDR PsF_HDR PsF_SDR | Set the format of the signals to be output from [8/PM] of the [HD SDI OUT] connector. When [CCU MODE] is [1080/29.97PsF], [1080/23.98PsF] or [1080/25PsF]: PsF_HDR/PsF_SDR When [CCU MODE] is other than [1080/29.97PsF], [1080/23.98PsF], [1080/25PsF]: HD_HDR/HD_SDR “Output selection conditions”
SDI OUT8 NORMAL/PM | PM NORMAL | Set the signal to be output from [8/PM] of the [HD SDI OUT] connector. Can only be set to PM when using a MoIP board (AK-NP600). PM : Output the picture monitor images. NORMAL : Output the main line images.
3G SDI | LEVEL-A LEVEL-B | Set the output format for 3G output.
HDR COLORIMETRY | BT.709 BT.2020 | Change the Y/C conversion coefficient.

#### Output selection conditions

FORMAT / CCU MODE | SDI | ANALOG
--- | --- | ---
OUT1 | OUT2 | OUT3 | OUT4 | OUT5 | OUT6 | OUT7 | OUT8 | COMPOSITE /PM
HD_HDR (59.94)
| 1080 /59.94p | 3G_HDR, HD_HDR, HD_SDR | HD_HDR, HD_SDR | NORMAL /PM
1080 /29.97PsF | HD_HDR, HD_SDR | PsF_HDR, PsF_SDR, TrueP_HDR, TrueP_SDR, OVER(3G)_HDR, OVER(3G)_SDR | PsF_HDR, PsF_SDR | NORMAL /PM
1080 /23.98PsF | HD_HDR, HD_SDR | PsF_HDR, PsF_SDR, TrueP_HDR, TrueP_SDR, OVER(3G)_HDR, OVER(3G)_SDR | PsF_HDR, PsF_SDR | NORMAL /PM
1080 /23.98p over 59.94i | HD_HDR, HD_SDR | HD_HDR, HD_SDR | NORMAL /PM
1080 /23PsF & over59i | HD_HDR, HD_SDR | HD_HDR, HD_SDR | NORMAL /PM
720 /59.94p | HD_HDR, HD_SDR | HD_HDR, HD_SDR | NORMAL /PM
HD_HDR (50)
| 1080 /50p | 3G_HDR, HD_HDR, HD_SDR | HD_HDR, HD_SDR | NORMAL /PM
1080 /25PsF | HD_HDR, HD_SDR | PsF_HDR, PsF_SDR, TrueP_HDR, TrueP_SDR, OVER(3G)_HDR, OVER(3G)_SDR | PsF_HDR, PsF_SDR | NORMAL /PM
720 /50p | HD_HDR, HD_SDR | HD_HDR, HD_SDR | NORMAL /PM

#### With AK-NP600 option

FORMAT / CCU MODE | SDI | SFP+
--- | --- | ---
OUT1 | OUT2 | OUT3 | OUT4 | OUT5 | OUT6 | OUT7 | OUT8 | 1 / 2
HD_HDR (59.94)
| 1080 /59.94p | 3G_HDR, HD_HDR, HD_SDR | HD_HDR, HD_SDR | 3G_HDR /HD_HDR /HD_SDR
1080 /23PsF & over59i | HD_HDR, HD_SDR | HD_HDR, HD_SDR | no signal
1080 /23.98p over 59.94i | HD_HDR, HD_SDR | HD_HDR, HD_SDR | no signal
1080 /29.97PsF | HD_HDR, HD_SDR | PsF_HDR, PsF_SDR, TrueP_HDR, TrueP_SDR, OVER_HDR, OVER_SDR | PsF_HDR, PsF_SDR | no signal
1080 /23.98PsF | HD_HDR, HD_SDR | PsF_HDR, PsF_SDR, TrueP_HDR, TrueP_SDR, OVER_HDR, OVER_SDR | PsF_HDR, PsF_SDR | no signal
720 /59.94p | HD_HDR, HD_SDR | HD_HDR, HD_SDR | HD
HD_HDR (50)
| 1080 /50p | 3G_HDR, HD_HDR, HD_SDR | HD_HDR, HD_SDR | 3G/HD PM
1080 /25PsF | HD_HDR, HD_SDR | PsF_HDR, PsF_SDR, TrueP_HDR, TrueP_SDR, OVER_HDR, OVER_SDR | PsF_HDR, PsF_SDR | no signal
720 /50p | HD_HDR, HD_SDR | HD_HDR, HD_SDR | HD

Top of the page