- Top
- CCU menu
- OPERATION
- OUT FORMAT(HS)

# OUT FORMAT(HS)

This is the selection screen for the OUT FORMAT (HS) menu.

- This is not displayed when AK-PLV100 is connected.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
SDI OUT1-4 | HS_3G HS_HD | Displays the format of the signals to be output from [1] to [4] of the [UHD/HS/HD SDI OUT] connectors.
SDI OUT5&6 | 3G HD | Set the format of the signals to be output from [5] to [6] of the [HD SDI OUT] connectors.
SDI OUT7 | 3G HD | Set the format of the signals to be output from [7] of the [HD SDI OUT] connector.
SDI OUT8 | HD | Displays the format of the signals to be output from [8/PM] of the [HD SDI OUT] connectors. (fixed)
SDI OUT8 NORMAL/PM | PM NORMAL | Set the signal to be output from [8/PM] of the [HD SDI OUT] connector. Can only be set to PM when using a MoIP board (AK-NP600). PM : Output the picture monitor images. NORMAL : Output the main line images.
3G SDI | LEVEL-A LEVEL-B | Set the output format for 3G output.
HD SDI FORMAT | 1080i 720P | Set the format for HD output.

#### Output selection conditions

FORMAT/ CCU MODE | SDI | ANALOG
--- | --- | ---
OUT1 | OUT2 | OUT3 | OUT4 | OUT5 | OUT6 | OUT7 | OUT8 | COMPOSITE /PM
UHD (59.94)
| 1080 /59.94p- 240fps | HS_3G, HS_HD | 3G, HD | HD | NORMAL /PM
1080 /59.94p- 180fps | HS_3G, HS_HD | no signal | 3G, HD | HD | NORMAL /PM
1080 /59.94p- 120fps | HS_3G, HS_HD | no signal | 3G, HD | HD | NORMAL /PM
720 /59.94p- 240fps | HD | HD | NORMAL /PM
720 /59.94p- 180fps | HD | no signal | HD | NORMAL /PM
720 /59.94p- 120fps | HD | no signal | HD | NORMAL /PM
HS (50)
| 1080 /50p-200fps | HS_3G, HS_HD | 3G, HD | HD | NORMAL /PM
1080 /50p-150fps | HS_3G, HS_HD | no signal | 3G, HD | HD | NORMAL /PM
1080 /50p-100fps | HS_3G, HS_HD | no signal | 3G, HD | HD | NORMAL /PM
720 /50p-200fps | HD | HD | NORMAL /PM
720 /50p-150fps | HD | no signal | HD | NORMAL /PM
720 /50p-100fps | HD | no signal | HD | NORMAL /PM

Top of the page