- Top
- CCU menu
- AUDIO
- CCU INTERCOM RECEIVE

# CCU INTERCOM RECEIVE

This is the selection screen for the CCU INTERCOM RECEIVE menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
CCU INCOM VR MIN MD | MUTE MIN_GAIN | Set the minimum intercom volume level.
PGM VR MIN MODE | MUTE MIN_GAIN | Set the minimum PGM volume level.
CCU INCOM OUT GAIN | Normal Boost | Switch the intercom output level.
ENG MIX CH2 | ON OFF | Set whether to mix the ENG signal with the intercom's CH2 output.
PROD MIX CH2 | ON OFF | Set whether to mix the PROD signal with the intercom's CH2 output.
PGM1 MIX CH2 | ON OFF | Set whether to mix the PGM1 signal with the intercom's CH2 output.
PGM2 MIX CH2 | ON OFF | Set whether to mix the PGM2 signal with the intercom's CH2 output.

Top of the page