- Top
- Web Screen
- [Setup] screen
- [Maintenance] screen

# [Maintenance] screen

Among the various maintenance operations performed on this screen are system log checks, software version check and initialization of the unit.

The Maintenance screen consists of three tabs: [Product info.], [Default reset] and [Back up].

#### [Product info.] tab

The versions of the unit's software can be checked on this screen.

The [Model no.], [MAC address], [Firmware version] and other information about the unit is displayed.

Item | Display description
--- | ---
Model no. | Display the unit's model number.
MAC address | Display the unit's MAC address.
Firmware version | CPU Software - SOFTWARE Display the software version of this unit. CPU Software - NETWORK Display the software version of the network. FPGA - UHD FPGA Display the image processing (4K) FPGA version. FPGA - HS FPGA Display the image processing (HS) FPGA version. FPGA - RETURN FPGA1 Display the return image processing FPGA1 version. FPGA - RETURN FPGA2 Display the return image processing FPGA2 version. FPGA - MAIN FPGA Display the FPGA version of this unit. FPGA - INCOM FPGA Display the power and audio management FPGA version. FPGA - USC FPGA Display the UHD output conversion FPGA version.
Viewer software installation counter | The number of plug-in viewer software applications which have been installed automatically from the unit is displayed by this counter.

#### [Default reset] tab

The unit's setting data or HTML is initialized and the unit is restarted on this screen.

Item | Setting details
--- | ---
Reset to the default (Except the network settings) | When the [Execute] button is clicked, the unit's settings are returned to their defaults. The login user name and password will also return to their defaults (admin/12345). When the initialization operation is started, no operations can be undertaken for about 3 minutes. The following setting items will not be returned to defaults. All settings under [IPv4 network] [HTTP port] [Line speed] [Bandwidth control (bit rate)]

#### [Back up] tab

On this screen, the unit's network settings can be saved to a personal computer or settings stored on a personal computer can be applied on the unit.

Item | Setting details
--- | ---
Download | Save the unit's network settings to a personal computer. “Saving the unit's network settings to a personal computer [Download]”
Upload | Upload a unit configuration file that was saved to a personal computer with the download function. “Applying settings stored on a personal computer to the unit [Upload]”

#### Saving the unit's network settings to a personal computer [Download]

Follow the procedure below to save the unit's network settings to a personal computer.

- Do not turn off the unit's power during downloading.

- Do not attempt to perform any operations during downloading. Wait until downloading is completed.

1.Click the [Execute] button of [Download].

The save destination dialog box appears.

2.Specify the save destination folder and then click the [OK] button.

The data is saved.

#### Applying settings stored on a personal computer to the unit [Upload]

Follow the procedure below to upload a unit configuration file that was saved to a personal computer with the download function [Download] and then apply the settings on the unit.

- For the data to use for uploading, use a file downloaded with the unit.

Furthermore, do not change the extension (.ndt) of the downloaded file.

- Do not turn off the unit's power during uploading.

- Do not attempt to perform any operations during uploading. Wait until uploading is completed.

1.Click the [Browse] button of [Upload], and specify the downloaded software.

2.Click the [Execute] button.

A message dialog box appears.

3.Click the [OK] button.

Uploading begins.

A message dialog box appears when uploading completes.

4.Click the [OK] button.

The unit restarts automatically.

Top of the page