- Top
- Parts and their functions
- Rear panel 2

# Rear panel 2

1 | [LAN] connector | It is the LAN connector (RJ45) for connecting the ROP (AK-HRP1000 / AK-HRP1005 / AK-HRP1010 / AK-HRP1015 / AK-HRP250) with an IP connection. Use a switch hub and connect the devices with a 10BASE-T/100BASE-TX straight cable. This connector is for connecting a personal computer when configuring Web settings. “Web Screen”
2 | [AUX] connector | This connector is used for controlling a waveform monitor and external systems (down-convert system, MIC gain selection, alarm output, or tally output).
3 | [TRUNK] connector | This connector provides two systems for 2-way communication of camera trunk data (RS-422 and RS-232C).
4 | [COMMUNICATION] connector | This connector is for connecting the intercom signals and tally signals to the external system.
5 | [ROP] connector | This connector is for connecting a ROP (sold separately).
6 | [MSU] connector | This connector is for connecting an MSU (sold separately).
7 | [MIC1] and [MIC2] connectors | These connectors are for outputting the analog signals of microphones 1 and 2 of the camera. The microphone level is 0 dBm/600 Ω.
8 | [CAMERA] connector | This connector is for connecting the optical fiber multi cable (sold separately).
9 | Cooling fan | This is the unit's cooling fan.
10 | AC power socket | This socket is for inputting AC power. Connect the supplied power cable, and use a 3-prong outlet and ground the unit properly.
11 | [SIGNAL GND] terminal | Connect this to the system ground.

Top of the page