- Top
- Parts and their functions
- Rear panel 3 (with AK-NP600 option)

# Rear panel 3 (with AK-NP600 option)

1 | [UHD/HS/HD SDI OUT] connectors [1] to [4] | UHD (connects to the AK-UC4000 / AK-UC3000 / AK-UC3300 / AK-PLV100), HS and 3G-HD, HD video signal output connectors (BNC). Signals output can be selected from the CCU menu. “OUT FORMAT(UHD)” “OUT FORMAT(HD)” “OUT FORMAT(UHD_HDR)” “OUT FORMAT(HD_HDR)”
2 | [HD SDI PROMPT IN] connector | These connectors (BNC) are for inputting HD-SDI prompter signals.
3 | [HD TRUNK/TICO OUT] connector | This connector outputs the HD SDI TRUNK signal input or TICO to the camera.
4 | [SFP+1] slot | 10GBASE-LR transceiver (SPF+) slot for MoIP input/output.
5 | [SFP+2] slot | 10GBASE-LR transceiver (SPF+) slot for MoIP input/output.
6 | [LAN2] connector | This connector is for ROP (AK-HRP1000 / AK-HRP1005 / AK-HRP1010 / AK-HRP1015 / AK-HRP250).

Top of the page